{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":11,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B","2MXS40H3V1B2","2MXS40H2V1B","2MXS50H3V1B","2MXS50H3V1B2","2MXS50H2V1B"]
["Sound pressure level","Heating","","Nom.","ديسيبل أمبير","48","48","","50","50"]
["","Cooling","","Nom.","ديسيبل أمبير","47","47","","48","48"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1"]
["","حقيبة المسامير اللولبية","","","","1","1","","1","1"]
["","سدادة المصرف","","","","1","1","","1","1"]
["","مجموعة المخفض","","","","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Charge","","","kg","1.20","1.20","","1.60","1.60"]
["","النوع","","","","R-410A","R-410A","","R-410A","R-410A"]
["Piping connections","Level difference","IU - IU","Max.","م","7.5","7.5","","7.5","7.5"]
["","","IU - OU","Max.","م","15","15","","15","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)","","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)"]
["","طول الأنابيب الإجمالي","النظام","فعلي","م","30","30","","30","30"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","مم","765","765","","765","765"]
["","","","العمق","مم","285","285","","285","285"]
["","","","الارتفاع","مم","550","550","","550","550"]
["الوزن","الوحدة","","","kg","38","38","","42","42"]
["Power supply","الطور","","","","1~","1~","","1~","1~"]
["","Frequency","","","Hz","50","50","","50","50"]
["","Voltage","","","V","220-240","220-240","","220-240","220-240"]
["Notes","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["الأبعاد","الوحدة","","الارتفاع","مم","","","550","","","550"]
["","","","العرض","مم","","","765","","","765"]
["","","","العمق","مم","","","285","","","285"]
["الوزن","الوحدة","","","kg","","","38","","","42"]
["Compressor","Type","","","","","","ضاغط متأرجح محكم مانع للتسريب","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°CDB","","","10","","","10"]
["","","","Max.","°CDB","","","46","","","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","","","-15","","","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","","","15.5","","","15.5"]
["Sound pressure level","Cooling","","Nom.","ديسيبل أمبير","","","47","","","48"]
["","Heating","","Nom.","ديسيبل أمبير","","","48","","","50"]
["سائل تبريد","النوع","","","","","","R-410A","","","R-410A"]
["","السعة","","","kg","","","1.20","","","1.60"]
["","السعة","","","tCO2Eq","","","2.5","","","3.3"]
["","GWP","","","","","","2087.5","","","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","","","20","","","20"]
["Piping connections","Additional refrigerant charge","","","kg/m","","","0.02 (for piping length exceeding 20m)","","","0.02 (for piping length exceeding 20m)"]
["","Level difference","IU - OU","Max.","م","","","15","","","15"]
["","","IU - IU","Max.","م","","","7.5","","","7.5"]
["وصلات الأنابيب","طول الأنابيب الإجمالي","النظام","فعلي","م","","","30","","","30"]
["Standard Accessories","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["وحدة التزويد بالطاقة","الطور","","","","","","1~","","","1~"]
["Power supply","Frequency","","","Hz","","","50","","","50"]
["","Voltage","","","V","","","220-240","","","220-240"]
["Standard Accessories","Reducer assembly","","","","","","","","","1"]