{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":8,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXS-E"]
[]
[]
[]
[]
["","","","","","3MXS52E4V1B2","3MXS52E4V1B","3MXS52E3V1B"]
["Sound pressure level","Heating","","Nom.","dBA","47","47"]
["","Cooling","","Nom.","dBA","46","46"]
["Standard Accessories","دليل التركيب","","","","1","1"]
["","سدادة المصرف","","","","1","1"]
["","مجموعة المخفض","","","","1","1"]
["","لوحة ضبط اتجاه الهواء","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","4.2","4.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Charge","","","كغ","2.0","2.0"]
["","النوع","","","","R-410A","R-410A"]
["Operation range","Cooling","Ambient","Max.","°CDB","46","46"]
["","","","Min.","°CDB","-10","-10"]
["","Heating","Ambient","Max.","°مئوية مقياس الحوجلة الرطبة","18","18"]
["","","","Min.","°مئوية مقياس الحوجلة الرطبة","-15","-15"]
["Piping connections","Level difference","IU - IU","Max.","m","7.5","7.5"]
["","","IU - OU","Max.","m","15","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)","0.02 (for piping length exceeding 30m)"]
["","طول الأنابيب الإجمالي","النظام","فعلي","m","50","50"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","مم","936","936"]
["","","","العمق","مم","300","300"]
["","","","الارتفاع","مم","735","735"]
["الوزن","الوحدة","","","كغ","49","49"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230","230"]
["Notes","","","","","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية للحوجلة الجافة؛ طول الأنبوب المكافئ: 7.5 م","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية للحوجلة الجافة؛ طول الأنبوب المكافئ: 7.5 م"]
["","","","","","(2) - التدفئة: درجة الحرارة الداخلية 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة؛ الطول المكافئ للمواسير: 7.5 متر","(2) - التدفئة: درجة الحرارة الداخلية 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة؛ الطول المكافئ للمواسير: 7.5 متر"]
["","","","","","(3) - يحتوي على غازات الاحتباس الحراري المفلورة","(3) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["الأبعاد","الوحدة","","الارتفاع","مم","","","735"]
["","","","العرض","مم","","","936"]
["","","","العمق","مم","","","300"]
["الوزن","الوحدة","","","كغ","","","49"]
["Compressor","Type","","","","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°CDB","","","-10"]
["","","","Max.","°CDB","","","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","","","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","","","15.5"]
["Sound pressure level","Cooling","","Nom.","dBA","","","46"]
["","Heating","","Nom.","dBA","","","47"]
["سائل تبريد","النوع","","","","","","R-410A"]
["","السعة","","","كغ","","","2.0"]
["","السعة","","","tCO2Eq","","","4.2"]
["","GWP","","","","","","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","m","","","25"]
["Piping connections","Additional refrigerant charge","","","kg/m","","","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","m","","","15"]
["","","IU - IU","Max.","m","","","7.5"]
["وصلات الأنابيب","طول الأنابيب الإجمالي","النظام","فعلي","m","","","50"]
["Standard Accessories","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["","Air direction adjustment plate","","","","","","1"]
["وحدة التزويد بالطاقة","الطور","","","","","","1~"]
["Power supply","Frequency","","","Hz","","","50"]
["","Voltage","","","V","","","230"]