{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":8,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXS-E"]
[]
[]
[]
[]
["","","","","","5MXS90E3V3B2","5MXS90E3V3B","5MXS90E7V3B"]
["Sound pressure level","Heating","","Nom.","ديسيبل أمبير","52","52"]
["","Cooling","","Nom.","ديسيبل أمبير","52","52"]
["Standard Accessories","دليل التركيب","","","","1"]
["","سدادة المصرف","","","","1","1"]
["","مجموعة المخفض","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","6.2","6.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Charge","","","kg","2.99","2.99"]
["","النوع","","","","R-410A","R-410A"]
["Operation range","Cooling","Ambient","Max.","°CDB","46"]
["","","","Min.","°CDB","-10"]
["","Heating","Ambient","Max.","°مئوية مقياس الحوجلة الرطبة","18"]
["","","","Min.","°مئوية مقياس الحوجلة الرطبة","-15"]
["Piping connections","Level difference","IU - IU","Max.","م","7.5"]
["","","IU - OU","Max.","م","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)"]
["","طول الأنابيب الإجمالي","النظام","فعلي","م","75"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","mm","900","900"]
["","","","العمق","mm","320","320"]
["","","","الارتفاع","mm","770","770"]
["الوزن","الوحدة","","","kg","73","73"]
["Power supply","الطور","","","","1~","1~"]
["","Frequency","","","هرتز","50","50"]
["","Voltage","","","فولت","230","230"]
["Notes","","","","","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية للحوجلة الجافة؛ طول الأنبوب المكافئ: 7.5 م","(1) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية للحوجلة الجافة؛ طول الأنبوب المكافئ: 7.5 م"]
["","","","","","(2) - التدفئة: درجة الحرارة الداخلية 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة؛ الطول المكافئ للمواسير: 7.5 متر","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m"]
["","","","","","(3) - يحتوي على غازات الاحتباس الحراري المفلورة","(3) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["Standard Accessories","Installation manual","","","","","1","1"]
["Piping connections","Level difference","IU - IU","Max.","م","","7.5"]
["","","IU - OU","Max.","م","","15"]
["","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 30m)"]
["","طول الأنابيب الإجمالي","النظام","فعلي","م","","75"]
["Compressor","Type","","","","","Hermetically sealed swing compressor"]
["الأبعاد","الوحدة","","الارتفاع","mm","","","770"]
["","","","العرض","mm","","","900"]
["","","","العمق","mm","","","320"]
["الوزن","الوحدة","","","kg","","","73"]
["Compressor","Type","","","","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°CDB","","","-10"]
["","","","Max.","°CDB","","","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","","","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","","","15.5"]
["Sound pressure level","Cooling","","Nom.","ديسيبل أمبير","","","52"]
["","Heating","","Nom.","ديسيبل أمبير","","","52"]
["سائل تبريد","النوع","","","","","","R-410A"]
["","السعة","","","kg","","","2.99"]
["","السعة","","","tCO2Eq","","","6.2"]
["","GWP","","","","","","2087.5"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","","","25"]
["Piping connections","Additional refrigerant charge","","","kg/m","","","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","م","","","15"]
["","","IU - IU","Max.","م","","","7.5"]
["وصلات الأنابيب","طول الأنابيب الإجمالي","النظام","فعلي","م","","","75"]
["Standard Accessories","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["وحدة التزويد بالطاقة","الطور","","","","","","1~"]
["Power supply","Frequency","","","هرتز","","","50"]
["","Voltage","","","فولت","","","230"]