{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Power input","Heating","","Nom.","kW","0.106","0.149"]
["","Cooling","","Nom.","kW","0.106","0.149"]
["مروحة","الضغط الاستاتيكي الخارجي","","عالٍ","Pa","0","0","0","0"]
["","","","منخفض","Pa","0","0","0","0"]
["Cooling capacity","Total capacity","","Nom.","kW","","","12.10","13.00"]
["استطاعة التدفئة","الاستطاعة الإجمالية","","الإسمي","kW","","","13.5","15.5"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض","أبيض"]
["","المادة","","","","Galvanised steel","Galvanised steel"]
["الأبعاد","الوحدة","","الارتفاع","mm","260","260","260","285"]
["","","","العرض","mm","1320","1538","1790","1900"]
["","","","العمق","mm","634","634","634","680"]
["الوزن","الوحدة","","","kg","38","45","65","70"]
["Fan","Air flow rate","التبريد","High","م³/دقيقة","23.8","31.1","34.4","43.9"]
["","","","Nom.","م³/دقيقة","21.3","27.8","31","39"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","م³/دقيقة","","","31","39"]
["Fan","Air flow rate","التبريد","Low","م³/دقيقة","18.9","24.8","27.2","28.3"]
["","","التدفئة","High","م³/دقيقة","23.8","31.1","34.4","43.9"]
["","","","Nom.","م³/دقيقة","21.3","27.8","30.6","39.1"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","م³/دقيقة","","","30.6","39.1"]
["Fan","Air flow rate","التدفئة","Low","م³/دقيقة","18.9","24.8","27.2","28.3"]
["مروحة","الضغط الاستاتيكي الخارجي","","الإسمي","Pa","0","0","0","0"]
["مستوى طاقة الصوت","التبريد","","","ديسيبل أمبير","59","64","65","71"]
["","التدفئة","","","ديسيبل أمبير","62","64","65","71"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","49","52","52","56"]
["","","","Nom.","ديسيبل أمبير","48","47"]
["مستوى ضغط الصوت","تبريد","","متوسط","ديسيبل أمبير","","","50","53"]
["Sound pressure level","Cooling","","Low","ديسيبل أمبير","46","46","49","46"]
["","Heating","","High","ديسيبل أمبير","49","52","52","56"]
["مستوى ضغط الصوت","تدفئة","","متوسط","ديسيبل أمبير","","","50","53"]
["Sound pressure level","Heating","","Nom.","ديسيبل أمبير","48","47"]
["","","","Low","ديسيبل أمبير","46","46","49","46"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.88","15.88","15.9","15.9"]
["","التصريف","","","","19.05","19.05"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","جهاز تحكم عن بُعد سلكي","","","","ARCWB","ARCWB"]
["Standard Accessories","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","أنبوب الصرف","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","فولت","220-240","220-240"]