{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Sound pressure level","Heating","","Nom.","dBA","","49.0"]
["","Cooling","","Nom.","dBA","","49.0"]
["Standard Accessories","سدادة المصرف","","","","","1"]
["","دليل التركيب","","","","","1"]
["","ملصق الشحن بسائل التبريد","","","","","1"]
["","ملصقات متعددة اللغات حول غازات الدفيئة المفلورة","","","","","1"]
["","تدابير السلامة الوقائية العامة","","","","","1"]
["Refrigerant","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","السعة","","","كغ","","0.76"]
["","النوع","","","","","R-32"]
["Operation range","Cooling","Ambient","Max.","°مئوية مقياس الحوجلة الجافة","","50 (4), 46 (5)"]
["","","","Min.","°مئوية مقياس الحوجلة الجافة","","-10"]
["Piping connections","Level difference","IU - OU","Max.","م","","15"]
["","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 10m)"]
["Compressor","Type","","","","","Hermetically sealed swing compressor"]
["Dimensions","Unit","","العرض","مم","","840"]
["","","","العمق","مم","","350"]
["","","","الارتفاع","مم","","552"]
["الوزن","الوحدة","","","كغ","","32"]
["Power supply","Phase","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]
["Notes","","","","","(1) - ممكن فقط كتركيبة مع ATXM*N2V1B، وFTXM*N2V1B، وATXM*R2V1B، وATXM*R5V1B، وFTXM*R2V1B، وFTXM*R5V1B","(1) - يحتوي على غازات الاحتباس الحراري المفلورة"]
["","","","","","(2) - ممكن فقط كتركيبة مع ATXM*M2V1B، وFTXM*M2V1B، وFVXM*FV1B، وFCAG*AVEB، وFFA*A2VEB9، وFBA*A2VEB9، وFHA*AVEB9، وFDXM*F3V1B9، وFNA*A2VEB9، وADEA*A2VEB، وFVXM*A2V1B","(2) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","","(3) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","","(4) - ممكن فقط كتركيبة مع ATXM*N2V1B، وFTXM*N2V1B، وATXM*R2V1B، وATXM*R5V1B، وFTXM*R2V1B، وFTXM*R5V1B"]
["","","","","","","(5) - ممكن فقط كتركيبة مع ATXM*M2V1B، وFTXM*M2V1B، وFVXM*FV1B، وFCAG*AVEB، وFFA*A2VEB9، وFBA*A2VEB9، وFHA*AVEB9، وFDXM*F3V1B9، وFNA*A2VEB9، وADEA*A2VEB، وFVXM*A2V1B"]
["الأبعاد","الوحدة","","الارتفاع","مم","552"]
["","","","العرض","مم","840"]
["","","","العمق","مم","350"]
["الوزن","الوحدة","","","كغ","32"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°مئوية مقياس الحوجلة الجافة","-10"]
["","","","Max.","°مئوية مقياس الحوجلة الجافة","50 (4), 46 (5)"]
["Sound pressure level","Cooling","","Nom.","dBA","46.0"]
["","Heating","","Nom.","dBA","47.0"]
["سائل تبريد","السعة","","","كغ","0.76"]
["","السعة","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","20"]
["Piping connections","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","م","15"]
["Standard Accessories","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Power supply","Frequency","","","Hz","50"]