{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-N / ARXM-R"]
[]
[]
[]
[]
["","","","","ATXM25N2V1B / ARXM25R5V1B","ATXM35N2V1B / ARXM35R5V1B"]
["Outdoor unit","","","","ARXM25R5V1B","ARXM35R5V1B"]
["Cooling capacity","Min.","","كيلوواط","1.30","1.40"]
["","Nom.","","كيلوواط","2.50","3.40"]
["","Max.","","كيلوواط","3.20","4.00"]
["Heating capacity","Min.","","كيلوواط","1.30","1.40"]
["","Nom.","","كيلوواط","2.80","4.00"]
["","Max.","","كيلوواط","4.70","5.20"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","4.39","4.09"]
["","عامل الأداء","","","5.00","4.04"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي","285","416"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A","A"]
["","","تدفئة","","A","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A+++","A+++"]
["","الاستطاعة","Pdesign","كيلوواط","2.50","3.40"]
["","SEER","","","8.55","8.55"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","102","139"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A+++","A+++"]
["","الاستطاعة","Pdesign","كيلوواط","2.40","2.50"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","5.10","5.10"]
["","Pdh استطاعة التدفئة عند -10°","","كيلوواط","2.30","2.35"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","659","687"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D","A+++ ~ D"]