{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MY1"]
[]
[]
[]
[]
["","","","","","AZAS100M7Y1B","AZAS125M7Y1B","AZAS140M7Y1B"]
["الأبعاد","الوحدة","","الارتفاع","مم","990","990","990"]
["","","","العرض","مم","940","940","940"]
["","","","العمق","مم","320","320","320"]
["الوزن","الوحدة","","","كغ","","70"]
["Compressor","Type","","","","","ضاغط متأرجح محكم مانع للتسريب"]
["Operation range","Cooling","Ambient","Min.","°CDB","-5","-5","-5"]
["","","","Max.","°CDB","46","46","46"]
["","Heating","Ambient","Min.","°مئوية مقياس الحوجلة الرطبة","-15","-15","-15"]
["","","","Max.","°مئوية مقياس الحوجلة الرطبة","15.5","15.5","15.5"]
["مستوى طاقة الصوت","التبريد","","","dBA","70","71","73"]
["","التدفئة","","","dBA","","71","73 (1)"]
["Sound pressure level","Cooling","","Nom.","dBA","53","53","54"]
["","Heating","","Nom.","dBA","57","57","57"]
["سائل تبريد","النوع","","","","R-32","R-32","R-32"]
["Refrigerant","Charge","","","كغ","","2.60"]
["","GWP","","","","","675"]
["سائل تبريد","السعة","","","tCO2Eq","1.76","1.76","1.96"]
["وصلات الأنابيب","سائل","","القطر الخارجي","مم","9.52","9.52","9.52"]
["Piping connections","غاز","","القطر الخارجي","مم","","15.9"]
["وصلات الأنابيب","طول الأنابيب","الحد الأعلى","الوحدة الخارجية - الوحدة الداخلية","م","30","30","30"]
["","","نظام","مكافئ","م","50","50","50"]
["","","","بدون شحن","م","30","30","30"]
["Piping connections","Additional refrigerant charge","","","kg/m","See installation manual","See installation manual","See installation manual"]
["","Level difference","IU - OU","Max.","م","30.0","30.0","30.0"]
["","","IU - IU","Max.","م","0.5","0.5","0.5"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["وحدة التزويد بالطاقة","الطور","","","","3~","3~","3~"]
["Power supply","Power supply-=-Frequency","","Frequency","","50","50","50"]
["","Power supply-=-Voltage","","Voltage","","380-415","380-415","380-415"]
["Current - 50Hz","Current - 50Hz-=-Maximum fuse amps (MFA)","","قيمة الأمبير القصوى للفاصمة (MFA)","","","16"]
["Notes","","","","","","(1) - حسب ENER Lot 21","(1) - حسب ENER Lot 21"]
["الوزن","الوحدة","","","كغ","70","","77"]
["ضاغط","نوع","","","","ضاغط متأرجح محكم مانع للتسريب","","ضاغط متأرجح محكم مانع للتسريب"]
["سائل تبريد","السعة","","","كغ","2.60","","2.90"]
["","GWP","","","","675","","675"]
["وصلات الأنابيب","غاز","","القطر الخارجي","مم","15.9","","15.9"]
["تيار - 50 هرتز","قيمة الأمبير القصوى للفاصمة (MFA)","","","A","16","","16"]