{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["مدخل الطاقة","كيلو واط","","","","0.015"]
["Maximum number of connectable indoor units","","","","","32"]
["الحد الأعلى لعدد الوحدات الخارجية القابلة للتوصيل @","","","","","7"]
["الأبعاد","الوحدة","","الارتفاع","مم","136"]
["","","","العرض","مم","384"]
["","","","العمق","مم","92"]
["الاتصال","DIII-NET","","الكمية","","1"]
["","","","ملاحظة","","DIII-NET (F1F2)"]
["","Ethernet","","الكمية","","1"]
["","محطة الإدخال الطرفية","رقمي","الكمية","","4"]
["Ambient temperature","Operation","","Min.","درجة مئوية","-10"]
["","","","Max.","درجة مئوية","50"]
["","المخزن","","Min.","درجة مئوية","-20"]
["","","","Max.","درجة مئوية","60"]
["درجة حرارة الوسط المحيط","درجة حرارة الوسط المحيط-=-الرطوبة النسبية <-=-%","","","%","85"]
["Power supply","Frequency","","","Hz","50/60"]
["","Voltage","","","V","تيار متناوب 110-240"]
["Notes","","","","","(1) - تتضمن مدخل الطاقة الخاص بوحدة التزويد بالطاقة WAGO ، ووحدة المعالجة المركزية ووحدة I/O"]
["","","","","","(2) - الأبعاد تشمل وحدة التزويد بالطاقة WAGO، ووحدة المعالجة المركزية، ووحدة I/O والمساحة الضرورية بين مختلف الأجزاء"]
["","","","","","(3) - أبعاد الشاشة الاختيارية هي: الارتفاع: 209مم، العرض: 123مم، العمق: 8.5مم"]