{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-CB / ERHQ-BW17"]
[]
[]
[]
[]
["","","","","EHBH16CB3V / ERHQ014BAW17","EHBH16CB9W / ERHQ014BAW17"]
["COP","","","","4.24 (1), 3.22 (2)","4.24 (1), 3.22 (2)"]
["Heating capacity","Nom.","","kW","14.5 (1), 13.6 (2)","14.5 (1), 13.6 (2)"]
["Power input","Heating","Nom.","kW","3.42 (1), 4.21 (2)","3.42 (1), 4.21 (2)"]
["Notes","","","","(1) - الحالة 1: التبريد Ta‏ 35‏° مئوية  - LWE‏ 18‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏ = 5‏° مئوية)","(1) - الحالة 1: التبريد Ta‏ 35‏° مئوية  - LWE‏ 18‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 35‏° مئوية (DT‏ = 5‏° مئوية)"]
["","","","","(2) - الحالة 2: التبريد Ta‏ 35‏° مئوية  - LWE‏ 7‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (DT‏ = 5‏° مئوية)","(2) - الحالة 2: التبريد Ta‏ 35‏° مئوية  - LWE‏ 7‏° مئوية (DT‏ = 5‏° مئوية)؛ التدفئة Ta الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (DT‏ = 5‏° مئوية)"]
["","","","","(3) - Tamb‏ 35‏° مئوية - LWE‏ 7‏° مئوية (DT‏=5‏°مئوية)","(3) - Tamb‏ 35‏° مئوية - LWE‏ 7‏° مئوية (DT‏=5‏°مئوية)"]
["","","","","(4) - Tamb‏ 35‏° مئوية - LWE‏ 18‏° مئوية (DT‏=5‏°مئوية)","(4) - Tamb‏ 35‏° مئوية - LWE‏ 18‏° مئوية (DT‏=5‏°مئوية)"]
["","","","","(5) - درجة حرارة الهواء الجاف/ درجة حرارة الهواء الرطب 7 درجة مئوية/ 6 درجة مئوية – LWC 35 درجة مئوية (درجة التكثف = 5 درجة مئوية)","(5) - درجة حرارة الهواء الجاف/ درجة حرارة الهواء الرطب 7 درجة مئوية/ 6 درجة مئوية – LWC 35 درجة مئوية (درجة التكثف = 5 درجة مئوية)"]
["","","","","(6) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (Dt‏=5‏° مئوية)","(6) - الحوجلة الجافة/الرطبة‏ 7‏° مئوية/6‏° مئوية - LWC‏ 45‏° مئوية (Dt‏=5‏° مئوية)"]