{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWET-BV3"]
[]
[]
[]
[]
["","","","","","EKHWET90BAV3","EKHWET120BAV3"]
["Mounting","","","","","Wall","Wall"]
["الغلاف","اللون","","","","أبيض + أسود","أبيض + أسود"]
["","المادة","","","","صفائح معدنية, Acrylonitrile Butadiene Styrene","صفائح معدنية, Acrylonitrile Butadiene Styrene"]
["الأبعاد","الوحدة","الارتفاع","خزان","mm","1032","1283"]
["","","","العرض","mm","510","510"]
["","","","العمق","mm","570","570"]
["الوزن","Unit","","Empty","kg","43","47"]
["Tank","Water volume","","","l","89","118"]
["","Material","","","","Enamel coated steel acc. DIN4753TL2","Enamel coated steel acc. DIN4753TL2"]
["خزان","درجة حرارة الماء العظمى","","","درجة مئوية","75.0","75.0"]
["","فئة فعالية استهلاك الطاقة","","","","B","C"]
["Heat exchanger","Domestic hot water","","Quantity","","1","1"]
["","","","Tube material","","ألمنيوم","ألمنيوم"]
["","","","Operating pressure","bar","42","42"]
["Booster heater","Capacity","","","kW","1.2","1.2"]