{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / FAA71BUV1B / RZQG100L8Y1B","FAA71BUV1B / FAA71BUV1B / RZQG125L8Y1B","FAA100BUV1B / RZQG100L8Y1B","FAA71BUV1B / RZQG71L8Y1B","FAA100BUV1B / RZQG71L8Y1B"]
["Cooling capacity","Nom.","","kW","","","","6.80","6.80"]
["تبريد المساحة","SEER","","","","","","6.43","6.43"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","","","","371","371"]
["","الاستطاعة","Pdesign","kW","","","","6.80","6.80"]
["","فئة فعالية استهلاك الطاقة","","","","","","A++","A++"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","","","","6.33","6.33"]
["","SCOP/A","","","","","","4.02","4.02"]
["","فئة فعالية استهلاك الطاقة","","","","","","A+","A+"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","","","","2,205","2,205"]
["الفعالية الاسمية","نسبة فعالية استهلاك الطاقة","","","","","","3.40","3.40"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","","","","1,000"]
["","عامل الأداء","","","","","","3.70"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","","","A"]
["","","تدفئة","","","","","A"]
["Heating capacity","Nom.","","kW","","","","7.50"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","","","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","","","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر.","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","","","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]