{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["الغلاف","اللون","","","","أبيض","أبيض"]
["","المادة","","","","Resin","Resin"]
["الأبعاد","الوحدة","","الارتفاع","mm","290","340"]
["","","","العرض","mm","1050","1200"]
["","","","العمق","mm","269","262"]
["الوزن","الوحدة","","","kg","14","18"]
["Fan","Air flow rate","Cooling","High","m³/min","16.2","23"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","13.4","21.1"]
["Fan","Air flow rate","Cooling","Low","m³/min","12.1","18.7"]
["","","Heating","High","m³/min","16.9","23"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","14.2","20.9"]
["Fan","Air flow rate","Heating","Low","m³/min","12.7","18.7"]
["مستوى طاقة الصوت","التبريد","","","ديسيبل أمبير","61","65"]
["","التدفئة","","","ديسيبل أمبير","61","65"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","45","49"]
["مستوى ضغط الصوت","تبريد","","متوسط","ديسيبل أمبير","42","45"]
["Sound pressure level","Cooling","","Low","ديسيبل أمبير","40","41"]
["","Heating","","High","ديسيبل أمبير","45","49"]
["مستوى ضغط الصوت","تدفئة","","متوسط","ديسيبل أمبير","42","45"]
["Sound pressure level","Heating","","Low","ديسيبل أمبير","40","41"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.9","15.9"]
["","التصريف","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~"]
["Power supply","Frequency","","","هرتز","50","50"]
["","Voltage","","","فولت","220-240","220-240"]
["Standard Accessories","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Notes","","","","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0"]
["","","","","","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["Standard Accessories","Screw cover","","","","","3"]