{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FBA35A2VEB / FBA35A2VEB / RZQSG71L3V1B","FBA50A2VEB / FBA50A2VEB / RZQSG100L9V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQSG100L9V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQSG125L9V1B","FBA50A2VEB / FBA50A2VEB / FBA50A2VEB / RZQSG125L9V1B","FBA60A2VEB / FBA60A2VEB / RZQSG125L9V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQSG140L9V1B","FBA71A2VEB / RZQSG71L3V1B"]
["تبريد المساحة","SEER","","","5.10","5.10","5.10","4.80","4.80","4.80","","5.84"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","467","652","652","875","875","875","","408"]
["","الاستطاعة","Pdesign","كيلوواط","6.80","9.50","9.50","12.0","12.0","12.0","","6.80"]
["","فئة فعالية استهلاك الطاقة","","","A","A","A","B","B","B","","A+"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","كيلوواط","6.00","7.60","7.60","7.60","7.60","7.60","","6.00"]
["","SCOP/A","","","3.80","3.80","3.80","3.80","3.80","3.80","","4.01"]
["","فئة فعالية استهلاك الطاقة","","","A","A","A","A","A","A","","A+"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","2,211","2,800","2,800","2,800","2,800","2,800","","2,095"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["Cooling capacity","Nom.","","كيلوواط","","9.50 (1)","","12.0 (1)","12.0 (1)","12.0 (1)","13.4 (1)","6.80 (1)"]
["الفعالية الاسمية","نسبة فعالية استهلاك الطاقة","","","","3.06 (3)","","3.04 (3)","2.94 (3)","2.83 (3)","4.20 (3)","3.43 (3)"]
["","عامل الأداء","","","","3.30 (3)","","3.35 (3)","3.30 (3)","3.26 (3)","","3.92 (3)"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","B","","B","C","C","","A"]
["","","تدفئة","","","C","","C","C","C","","A"]
["Heating capacity","Nom.","","كيلوواط","","10.8 (2)","","13.5 (2)","13.5 (2)","13.5 (2)","15.5 (2)","7.50 (2)"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلوواط ساعي","","","","","","","","991"]