{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB","FBA50A2VEB","FBA60A2VEB","FBA71A2VEB"]
["Sound pressure level","Heating","","High","ديسيبل أمبير","37.0","37.0","31.0","31.0"]
["","","","متوسط","ديسيبل أمبير","34.0","34.0","28.0","28.0"]
["","","","Low","ديسيبل أمبير","29.0","29.0","25.0","25.0"]
["","Cooling","","متوسط","ديسيبل أمبير","32.0","32.0","28.0","28.0"]
["","","","Low","ديسيبل أمبير","29.0","29.0","25.0","25.0"]
["","","","High","ديسيبل أمبير","35.0","35.0","30.0","30.0"]
["Standard Accessories","دليل التشغيل","","","","1","1","1","1"]
["","دليل التركيب","","","","1","1","1","1"]
["","خرطوم الصرف","","","","1","1","1","1"]
["","مشبك معدني لخرطوم الصرف","","","","1","1","1","1"]
["","حلقة للدعامة الحاملة","","","","8","8","8","8"]
["","مسامير لولبية","","","","40","40","40","40"]
["","عازل لأدوات التثبيت","","","","2","2","2","2"]
["","لباد مانع للتسريب","","","","5","5","5","5"]
["","مشابك","","","","4","4","4","4"]
["Control systems","Wired remote control","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Piping connections","Liquid","","القطر الخارجي","mm","6.35","6.35","6.35","9.52"]
["","غاز","","القطر الخارجي","mm","9.52","12.70","12.70","15.90"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","التبريد","","","ديسيبل أمبير","60","60","56","56"]
["Dimensions","Unit","","العرض","mm","700","700","1,000","1,000"]
["","","","العمق","mm","800","800","800","800"]
["","","","الارتفاع","mm","245","245","245","245"]
["Casing","Material","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["","Colour","","","","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)"]
["الوزن","الوحدة","","","كغ","28.0","28.0","35.0","35.0"]
["Fan","External static pressure","","عالٍ","باسكال","150","150","150","150"]
["","","","الإسمي","باسكال","30","30","30","30"]
["","Air flow rate","التدفئة","High","م³/دقيقة","15.0","15.0","18.0","18.0"]
["","","","Low","م³/دقيقة","10.5","10.5","12.5","12.5"]
["","","","متوسط","م³/دقيقة","12.5","12.5","15.0","15.0"]
["","","التبريد","Low","م³/دقيقة","10.5","10.5","12.5","12.5"]
["","","","متوسط","م³/دقيقة","12.5","12.5","15.0","15.0"]
["","","","High","م³/دقيقة","15.0","15.0","18.0","18.0"]
["ارتفاع الصرف","mm","","","","625","625","625","625"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","هرتز","50/60","50/60","50/60","50/60"]
["","Voltage","","","فولت","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت."]
["","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]