{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FBQ50C8VEB / FBQ50C8VEB / RZQSG100L8Y1B","FBQ100C8VEB / RZQSG100L8Y1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG100L8Y1B","FBQ125C8VEB / RZQSG125L8Y1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG125L8Y1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQSG125L8Y1B","FBQ60C8VEB / FBQ60C8VEB / RZQSG125L8Y1B","FBQ140C8VEB / RZQSG140L7Y1B"]
["Cooling capacity","Nom.","","كيلوواط","","9.5","","12.0","","","","13.4"]
["تبريد المساحة","SEER","","","5.1","5.5","5.1","5.2","4.8","4.8","4.8"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","652","605","652","808","875","875","875"]
["","الاستطاعة","Pdesign","كيلوواط","9.5","9.5","9.5","12","12","12","12"]
["","فئة فعالية استهلاك الطاقة","","","B","A","B","A","B","B","B"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","كيلوواط","7.6","7.6","7.6","7.6","7.6","7.6","7.6"]
["","SCOP/A","","","3.8","4.01","3.8","3.9","3.8","3.8","3.8"]
["","فئة فعالية استهلاك الطاقة","","","A","A+","A","A","A","A","A"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","2,800","2,654","2,800","2,729","2,800","2,800","2,800"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","","1,435","","1,870","","","","2,220"]
["","نسبة فعالية استهلاك الطاقة","","","","3.31","","3.21","","","","3.02"]
["","عامل الأداء","","","","3.65","","3.51","","","","3.41"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","A","","A"]
["","","تدفئة","","","A","","B"]
["Heating capacity","Nom.","","كيلوواط","","10.8","","13.5","","","","15.5"]
["Notes","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]