{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":23,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG71L8Y1B","FBQ35D2VEB / FBQ35D2VEB / RZQG71L8Y1B","FBQ71D2VEB / RZQG71L8Y1B","FBQ100D2VEB / RZQG71L8Y1B","FBQ50D2VEB / FBQ50D2VEB / RZQG71L8Y1B","FBQ140D2VEB / RZQG100L8Y1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG100L8Y1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQG100L8Y1B","FBQ71D2VEB / FBQ71D2VEB / RZQG100L8Y1B","FBQ100D2VEB / RZQG100L8Y1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG100L8Y1B","FBQ50D2VEB / FBQ50D2VEB / RZQG100L8Y1B","FBQ125D2VEB / RZQG125L8Y1B","FBQ140D2VEB / RZQG125L8Y1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQG125L8Y1B","FBQ60D2VEB / FBQ60D2VEB / RZQG125L8Y1B","FBQ71D2VEB / FBQ71D2VEB / RZQG125L8Y1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG125L8Y1B","FBQ140D2VEB / RZQG140L7Y1B"]
["Cooling capacity","Nom.","","kW","","","6.8 (2)","","","","","","","9.5 (2)","","","12.0 (2)","","","","","","13.4 (2)"]
["تبريد المساحة","SEER","","","5.10","5.10","6.16","6.16","5.10","5.87","5.10","5.10","5.10","5.87","5.10","5.10","6.11","6.11","5.10","5.10","5.10","5.10"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","466","466","386","386","466","566","652","652","652","566","652","652","687","687","824","824","824","824"]
["","الاستطاعة","Pdesign","kW","6.80","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","12.00"]
["","فئة فعالية استهلاك الطاقة","","","A","A","A++","A++","A","A+","A","A","A","A+","A","A","A++","A++","A","A","A","A"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","6.00","6.00","6.00","6.00","6.00","11.30","11.30","11.30","11.30","11.30","11.30","11.30","12.70","12.70","12.71","12.71","12.71","12.71"]
["","SCOP/A","","","3.80","3.80","4.31","4.31","3.80","4.78","3.80","3.80","3.80","4.78","3.80","3.80","4.28","4.28","3.80","3.80","3.80","3.80"]
["","فئة فعالية استهلاك الطاقة","","","A","A","A+","A+","A","A++","A","A","A","A++","A","A","A+","A+","A","A","A","A"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","2,210","2,210","1,949","1,949","2,210","3,310","4,163","4,163","4,163","3,310","4,163","4,163","4,154","4,154","4,683","4,683","4,683","4,683"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلوواط ساعي","","","944","","","","","","","1,247","","","1,813"]
["","نسبة فعالية استهلاك الطاقة","","","","","3.60 (1)","","","","","","","3.81 (1)","","","3.31 (1)","","","","","","3.35 (1)"]
["","عامل الأداء","","","","","4.01 (1)","","","","","","","4.41 (1)","","","3.90 (1)","","","","","","3.60 (1)"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","","A","","","","","","","A","","","A"]
["","","تدفئة","","","","A","","","","","","","A","","","A"]
["Heating capacity","Nom.","","kW","","","7.50 (2)","","","","","","","10.80 (2)","","","13.50 (2)","","","","","","15.50 (2)"]
["Notes","","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","","","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]