{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":12,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D"]
[]
[]
[]
[]
["","","","","","FBQ35D2VEB","FBQ50D2VEB","FBQ60D2VEB","FBQ71D2VEB","FBQ100D2VEB","FBQ125D2VEB","FBQ140D2VEB"]
["Sound pressure level","Heating","","High","ديسيبل أمبير","37","37","31","31.0","36.0","38.0","38"]
["","","","متوسط","ديسيبل أمبير","34","34","28","28.0","33.0","35.0","35"]
["","","","Low","ديسيبل أمبير","29","29","25","25.0","30.0","32.0","32"]
["","Cooling","","متوسط","ديسيبل أمبير","32","32","28","28.0","32.0","35.0","35"]
["","","","Low","ديسيبل أمبير","29","29","25","25.0","30.0","32.0","32"]
["","","","High","ديسيبل أمبير","35","35","30","30.0","34.0","37.0","37"]
["Standard Accessories","دليل التشغيل","","","","1","1","1","1","1","1","1"]
["","دليل التركيب","","","","1","1","1","1","1","1","1"]
["","خرطوم الصرف","","","","1","1","1","1","1","1","1"]
["","مشبك معدني لخرطوم الصرف","","","","1","1","1","1","1","1","1"]
["","حلقة للدعامة الحاملة","","","","8","8","8","8","8","8","8"]
["","مسامير لولبية","","","","40","40","40","40","40","40","40"]
["","عازل لأدوات التثبيت","","","","2","2","2","2","2","2","2"]
["","لبادة مانعة للتسريب","","","","5","5","5","5","5","5","5"]
["","لباد مانع للتسريب","","","","","","","5","5","5","5"]
["","مشابك","","","","4","4","4","4","4","4","4"]
["Refrigerant","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["أنظمة التحكم","Wired remote control","","","","","","","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528"]
["","Infrared remote control","","","","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Piping connections","Liquid","","القطر الخارجي","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","9.52","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Drain","","","","VP20 (قطر داخلي 20/قطر خارجي 26)، ارتفاع المصرف 625 مم","VP20 (قطر داخلي 20/قطر خارجي 26)، ارتفاع المصرف 625 مم","VP20 (قطر داخلي 20/قطر خارجي 26)، ارتفاع المصرف 625 مم","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","التبريد","","","ديسيبل أمبير","60","60","56","56","58","62","62"]
["Dimensions","Unit","","العرض","mm","700","700","1,000","1,000","1,400","1,400","1,400"]
["","","","العمق","mm","800","800","800","800","800","800","800"]
["","","","الارتفاع","mm","245","245","245","245","245","245","245"]
["الغلاف","المادة","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["","اللون","","","","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)"]
["الوزن","الوحدة","","","kg","28.0","28.0","35.0","35.0","46.0","46.0","46.0"]
["Fan","External static pressure","","عالٍ","باسكال","150","150","150","150","150","150","150"]
["","","","الإسمي","باسكال","30","30","30","30","40","50","50"]
["","Air flow rate","التدفئة","High","m³/min","","","","","29.0","34.0","34.0"]
["","","","Low","m³/min","","","","","23.0","23.5","23.5"]
["","","","متوسط","m³/min","","","","","26.0","29.0","29.0"]
["","","التبريد","Low","m³/min","","","","","23.0","23.5","23.5"]
["","","","متوسط","m³/min","","","","","26.0","29.0","29.0"]
["","","","High","m³/min","","","","","29.0","34.0","34.0"]
["ارتفاع الصرف","mm","","","","625","625","625","625","625","625","625"]
["Power supply","الطور","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","الاسم","","","","VE","VE","VE","VE","VE","VE","VE"]
["","Voltage","","","V","220-240","220-240","220-240","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(1) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت."]