{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / ARXM-N9"]
[]
[]
[]
[]
["","","","","FCAG71BVEB / ARXM71N2V1B9"]
["Cooling capacity","Nom.","","كيلو واط","6.80"]
["","Max.","","كيلو واط","7.05"]
["Heating capacity","Nom.","","كيلو واط","7.50"]
["","Max.","","كيلو واط","7.58"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","1,083"]
["","عامل الأداء","","","3.38"]
["","نسبة فعالية استهلاك الطاقة","","","3.14"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","B"]
["","","تدفئة","","C"]
["Notes","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0"]
["","","","","(4) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]