{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":23,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100BVEB / RZQG100L8Y1B","FCAG125BVEB / RZQG125L8Y1B","FCAG140BVEB / RZQG100L8Y1B","FCAG140BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG125L8Y1B","FCAG60BVEB / FCAG60BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG125L8Y1B","FCAG100BVEB / RZQG71L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG71BVEB / RZQG71L8Y1B","FCAG140BVEB / RZQG140L7Y1B"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Cooling capacity","Nom.","","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["الفعالية الاسمية","نسبة فعالية استهلاك الطاقة","","","","","","","","","","","","","","","","3.39","3.30","3.30","3.30","3.39","2.50"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","","","","","","","","","","","","","","A++","A","A","A","A++"]
["","الاستطاعة","Pdesign","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["","SEER","","","","","","","","","","","","","","","","6.80","5.10","5.10","5.10","6.72","6.44"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","","","","","","","","","","","","350","467","467","467","355","1,249"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","","","","","","","","","","","","","","A+","A","A","A","A+"]
["","الاستطاعة","Pdesign","kW","","","","","","","","","","","","","","6.33","6.00","6.00","6.00","6.33","11.56"]
["","SCOP/A","","","","","","","","","","","","","","","","4.20","3.80","3.80","3.80","4.20","4.27"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","","","","","","","","","","","","2,110","2,211","2,211","2,211","2,110","3,795"]
["Notes","","","","","","","","","","","","","","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م."]
["","","","","","","","","","","","","","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر.","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر.","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["","","","","","","","","","","","","","","","","","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","","","","","","","","","","","","","","","","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["Heating capacity","Nom.","","kW","","","","","","","","","","","","","","","","","","7.50","15.50"]
["الفعالية الاسمية","عامل الأداء","","","","","","","","","","","","","","","","","","","","3.97","3.61"]
["","استهلاك الطاقة السنوي","","kWh","","","","","","","","","","","","","","","","","","1,003"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","","","","","","","","","","","","","","","","","A"]
["","","تدفئة","","","","","","","","","","","","","","","","","","","A"]