{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZAG-NV1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZAG100N7V1B"]
["Cooling capacity","Nom.","","كيلوواط","9.50 (1)"]
["Heating capacity","Nom.","","كيلوواط","10.8 (2)"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A++"]
["","الاستطاعة","Pdesign","كيلوواط","9.50"]
["","SEER","","","7.35"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","452"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A++"]
["","الاستطاعة","Pdesign","كيلوواط","9.52"]
["","SCOP/A","","","4.81"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","2,771"]
["Notes","","","","(1) - التبريد: T2: درجة الحرارة الداخلية 26,6‏° مئوية CDB، و19,4‏° مئوية CWB، درجة الحرارة الخارجية 48°CDB [وحدة حرارية/ساعة/واط]"]
["","","","","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]