{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100HVEB / RZQG100L8Y1B","FCAHG125HVEB / RZQG125L8Y1B","FCAHG140HVEB / RZQG100L8Y1B","FCAHG140HVEB / RZQG125L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG100L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG125L8Y1B","FCAHG100HVEB / RZQG71L8Y1B","FCAHG71HVEB / RZQG71L8Y1B","FCAHG140HVEB / RZQG140L7Y1B"]
["Cooling capacity","Nom.","","kW","","","","","","","6.80","6.80","13.40"]
["تبريد المساحة","SEER","","","","","","","","","6.91","6.91","6.75"]
["","ηs,c","","%","","","","","","","","","266.88"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","","","","","345","345","1,191"]
["","الاستطاعة","Pdesign","kW","","","","","","","6.80","6.80","13.40"]
["","فئة فعالية استهلاك الطاقة","","","","","","","","","A++","A++"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","","","","","","","7.60","7.60","11.78"]
["","SCOP/A","","","","","","","","","4.54","4.54","4.38"]
["","فئة فعالية استهلاك الطاقة","","","","","","","","","A+","A+"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","","","","","2,344","2,344","3,766"]
["","ηs,h","","%","","","","","","","","","172.10"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","","","","","","","","831"]
["","نسبة فعالية استهلاك الطاقة","","","","","","","","","4.09","4.09","3.18"]
["","عامل الأداء","","","","","","","","","","4.80","4.12"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","","","","","","","A"]
["","","تدفئة","","","","","","","","","A"]
["Heating capacity","Nom.","","kW","","","","","","","","7.50","15.50"]
["Notes","","","","","","","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م."]
["","","","","","","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر.","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","","","","","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","","","","","","","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]