{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":21,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / FCQG35FVEB / RZQG71L9V1B","FCQG71FVEB / RZQG71L9V1B","FCQG100FVEB / RZQG71L9V1B","FCQG100FVEB / RZQG100L9V1B","FCQG140FVEB / RZQG100L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L9V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG100L9V1B","FCQG71FVEB / FCQG71FVEB / RZQG100L9V1B","FCQG50FVEB / FCQG50FVEB / RZQG100L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG125L9V1B","FCQG140FVEB / RZQG125L9V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG125L9V1B","FCQG60FVEB / FCQG60FVEB / RZQG125L9V1B","FCQG71FVEB / FCQG71FVEB / RZQG125L9V1B","FCQG125FVEB / RZQG125L9V1B","FCQG140FVEB / RZQG140L9V1B"]
["Cooling capacity","Nom.","","كيلوواط","","6.8","","9.5","","","","","","","","","","","","12.0","13.4"]
["تبريد المساحة","SEER","","","5.10","6.72","6.80","6.80","6.80","5.10","5.10","5.10","5.10","5.10","5.10","6.00","5.10","5.10","5.10","6.00"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","467","355","350","489","489","652","652","652","652","652","824","700","824","824","824","700"]
["","الاستطاعة","Pdesign","كيلوواط","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","12.00"]
["","فئة فعالية استهلاك الطاقة","","","B","A++","A++","A++","A++","B","B","B","B","B","B","A+","B","B","B","A+"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","كيلوواط","6.00","6.33","6.33","11.30","11.30","11.30","11.30","11.30","11.30","11.30","12.71","12.66","12.71","12.71","12.71","12.66"]
["","SCOP/A","","","3.80","4.20","4.20","4.61","4.61","3.80","3.80","3.80","3.80","3.80","3.80","4.10","3.80","3.80","3.80","4.10"]
["","فئة فعالية استهلاك الطاقة","","","A","A+","A+","A++","A++","A","A","A","A","A","A","A+","A","A","A","A+"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","2,211","2,110","2,110","3,432","3,432","4,164","4,164","4,164","4,164","4,164","4,683","4,323","4,683","4,683","4,683","4,323"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","","1,005","","1,225","","","","","","","","","","","","1,610"]
["","نسبة فعالية استهلاك الطاقة","","","","3.39","","3.87","","","","","","","","","","","","3.73","3.21"]
["","عامل الأداء","","","","3.97","","4.15","","","","","","","","","","","","3.63","3.61"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","A","","A","","","","","","","","","","","","A"]
["","","تدفئة","","","A","","A","","","","","","","","","","","","A"]
["Heating capacity","Nom.","","كيلوواط","","7.5","","10.8","","","","","","","","","","","","13.5","15.5"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","","(1) - يتوافق الاستهلاك السنوي للطاقة مع توجيه الطاقة الملصق 2002/31/EC","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","","","","","","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","","(2) - يتوافق SEER وSCOP مع EN 14825","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","","","","","","","","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]