{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":5,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A / RZASG-MV"]
[]
[]
[]
[]
["","","","","FDA125A5VEB / RZASG125MUV"]
["Cooling capacity","Nom.","","كيلوواط","12.1 (1)"]
["Heating capacity","Nom.","","كيلوواط","13.5 (2)"]
["تبريد المساحة","الاستطاعة","Pdesign","كيلوواط","12.1"]
["","SEER","","","5.03"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","1444"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","كيلوواط","6"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","3.58"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","2346"]
["Notes","","","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0"]
["","","","","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]