{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Cooling capacity","Total capacity","","Nom.","كيلوواط","12.10","19.00","22.00"]
["Heating capacity","الاستطاعة الإجمالية","","الإسمي","كيلوواط","13.50","22.4","24.0"]
["الغلاف","اللون","","","","Unpainted","Unpainted","Unpainted"]
["","المادة","","","","Galvanised steel","Galvanised steel plate","Galvanised steel plate"]
["Dimensions","Unit","","الارتفاع","مم","300","470","470"]
["","","","العرض","مم","1,400","1,490","1,490"]
["","","","العمق","مم","700","1,100","1,100"]
["الوزن","الوحدة","","","كغ","45","104","115"]
["مطلوب مسافة فوق السقف المستعار >","مم","","","","350"]
["Fan","Air flow rate","التبريد","High","م³/دقيقة","39.0","64.0","69.0"]
["","","","متوسط","م³/دقيقة","","50","56"]
["","","","Low","م³/دقيقة","28.0","36.0","43.0"]
["","","التدفئة","High","م³/دقيقة","39.0","64.0","69.0"]
["","","","متوسط","م³/دقيقة","","50.0","56.0"]
["","","","Low","م³/دقيقة","28.0","36.0","43.0"]
["","External static pressure","","عالٍ","باسكال","200","250","250"]
["","","","الإسمي","باسكال","50","62","62"]
["Sound power level","التبريد","","","ديسيبل أمبير","66","69.0","71.0"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","40","43.0","44.0"]
["","","","متوسط","ديسيبل أمبير","","39.0","40.0"]
["","","","Low","ديسيبل أمبير","33","36.0","37.0"]
["","Heating","","High","ديسيبل أمبير","40","43.0","44.0"]
["","","","متوسط","ديسيبل أمبير","","39.0","40.0"]
["","","","Low","ديسيبل أمبير","33","36.0","37.0"]
["Piping connections","Liquid","","القطر الخارجي","مم","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","مم","15.90","19.1","22.2"]
["","Drain","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["ارتفاع الصرف","مم","","","","625"]
["لوحة ديكور","الطراز","","","","BYBS125DJW1"]
["","اللون","","","","White (10Y9/0.5)"]
["","الأبعاد","","الارتفاع","مم","55"]
["","","","العرض","مم","1,500"]
["","","","العمق","مم","500"]
["","الوزن","","","كغ","6.5"]
["أنظمة التحكم","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standard Accessories","دليل التشغيل","","","","","1","1"]
["","دليل التركيب والتشغيل","","","","1","1","1"]
["","دليل التركيب","","","","","1","1"]
["","تدابير السلامة الوقائية العامة","","","","1","1","1"]
["","أنبوب توصيل الغاز","","","","","1","1"]
["","مادة مشبك السلك","","","","","1","1"]
["","حلقة إحكام الربط","","","","8","12","12"]
["","حلقة نابضية","","","","","2","2"]
["","برغي+حلقة","","","","","45","45"]
["","برغي برأس سداسي مع حلقة","","","","","49","49"]
["","مسامير لولبية","","","","16","2","2"]
["","برغي برأس سداسي","","","","","2","2"]
["","حلقة عادية","","","","","8","8"]
["Power supply","الاسم","","","","","VE","VE"]
["","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220"]
["Standard Accessories","حلقة تثبيت الخرطوم","","","","1"]
["","خرطوم الصرف","","","","1"]
["","سلك للوحدة العامة للتزويد بالطاقة","","","","2"]
["","مادة مانعة للتسريب (خرطوم تصريف)","","","","1"]
["","مواد مانعة للتسريب","","","","2"]
["","أنبوب عزل حراري (سائل)","","","","1"]
["","أنبوب عزل حراري (غاز)","","","","1"]
["Notes","","","","","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]