{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-E / RXS-K"]
[]
[]
[]
[]
["","","","","FDXS25E7VMB / RXS25K2V1B"]
["Cooling capacity","Nom.","","كيلوواط","2.40 (3)"]
["Piping connections","Liquid","القطر الخارجي","مم","6.35"]
["","غاز","القطر الخارجي","مم","9.5"]
["","Drain","OD","مم","VP20 (القطر الخارجي 26؛ القطر الداخلي 20)"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","345"]
["","نسبة فعالية استهلاك الطاقة","","","3.48"]
["","عامل الأداء","","","3.52"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","B"]
["Heating capacity","Nom.","","كيلوواط","3.20 (4)"]
["Notes","","","","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)"]
["","","","","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","(5) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]