{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXM50N2V1B","FFA60A2VEB / RXM60N2V1B"]
["Cooling capacity","Nom.","","kW","","5.70"]
["Heating capacity","Nom.","","kW","","7.00"]
["الفعالية الاسمية","نسبة فعالية استهلاك الطاقة","","","","3.05"]
["","عامل الأداء","","","","3.41"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","","934"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","B"]
["","","تدفئة","","","B"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","","A+"]
["","الاستطاعة","Pdesign","kW","","5.70"]
["","SEER","","","","5.76"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","347"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","","A+"]
["","الاستطاعة","Pdesign","kW","","3.96"]
["","SCOP/A","","","","4.04"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","1,372"]
["Notes","","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0"]
["","","","","","(4) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["Outdoor unit","","","","RXM50N2V1B"]
["Cooling capacity","Nom.","","kW","5.00"]
["Heating capacity","Nom.","","kW","5.80"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","3.24"]
["","عامل الأداء","","","3.49"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","771"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","B"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A+"]
["","الاستطاعة","Pdesign","kW","5.00"]
["","SEER","","","5.98"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","292"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A"]
["","الاستطاعة","Pdesign","kW","3.84"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","3.90"]
["","Pdh استطاعة التدفئة عند -10°","","kW","3.51"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","1377"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D"]