{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB","FFA35A2VEB","FFA50A2VEB","FFA60A2VEB"]
["الغلاف","المادة","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["الأبعاد","الوحدة","","الارتفاع","mm","260","260","260","260"]
["","","","العرض","mm","575","575","575","575"]
["","","","العمق","mm","575","575","575","575"]
["الوزن","الوحدة","","","كغ","16.0","16.0","17.5","17.5"]
["Fan","Air flow rate","التبريد","High","m³/min","9.0","10.0","12.0","14.5"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","8.0","8.5","10.0","12.5"]
["Fan","Air flow rate","التبريد","Low","m³/min","6.5","6.5","7.5","9.5"]
["","","التدفئة","High","m³/min","9.0","10.0","12.0","14.5"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","8.0","8.5","10.0","12.5"]
["Fan","Air flow rate","التدفئة","Low","m³/min","6.5","6.5","7.5","9.5"]
["مستوى طاقة الصوت","التبريد","","","ديسيبل أمبير","48","51","56","60"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","31.0","34.0","39.0","43.0"]
["مستوى ضغط الصوت","تبريد","","متوسط","ديسيبل أمبير","28.5","30.5","34.0","40.0"]
["Sound pressure level","Cooling","","Low","ديسيبل أمبير","25.0","25.0","27.0","32.0"]
["","Heating","","High","ديسيبل أمبير","31.0","34.0","39.0","43.0"]
["مستوى ضغط الصوت","تدفئة","","متوسط","ديسيبل أمبير","28.5","30.5","34.0","40.0"]
["Sound pressure level","Heating","","Low","ديسيبل أمبير","25.0","25.0","27.0","32.0"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.52","9.52","12.70","12.70"]
["","التصريف","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["لوحة ديكور","الطراز","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","اللون","","","","أبيض (N9.5)","أبيض (N9.5)","أبيض (N9.5)","أبيض (N9.5)"]
["","الأبعاد","","الارتفاع","mm","46","46","46","46"]
["","","","العرض","mm","620","620","620","620"]
["","","","العمق","mm","620","620","620","620"]
["","الوزن","","","كغ","2.8","2.8","2.8","2.8"]
["لوحة ديكور 2","الطراز","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","اللون","","","","فضة","فضة","فضة","فضة"]
["","الأبعاد","","الارتفاع","mm","46","46","46","46"]
["","","","العرض","mm","620","620","620","620"]
["","","","العمق","mm","620","620","620","620"]
["","الوزن","","","كغ","2.8","2.8","2.8","2.8"]
["لوحة ديكور 3","الطراز","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","اللون","","","","أبيض (RAL9010)","أبيض (RAL9010)","أبيض (RAL9010)","أبيض (RAL9010)"]
["","الأبعاد","","الارتفاع","mm","55","55","55","55"]
["","","","العرض","mm","700","700","700","700"]
["","","","العمق","mm","700","700","700","700"]
["","الوزن","","","كغ","2.7","2.7","2.7","2.7"]
["لوحة ديكور 4","الطراز","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","اللون","","","","أبيض (RAL9010)","أبيض (RAL9010)","أبيض (RAL9010)","أبيض (RAL9010)"]
["","الأبعاد","","الارتفاع","mm","55","55","55","55"]
["","","","العرض","mm","700","700","700","700"]
["","","","العمق","mm","700","700","700","700"]
["","الوزن","","","كغ","2.7","2.7","2.7","2.7"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","BRC7EB530 (لوحة قياسية), BRC7F530W (لوحة بيضاء), BRC7F530S (لوحة رمادية)","BRC7EB530 (لوحة قياسية), BRC7F530W (لوحة بيضاء), BRC7F530S (لوحة رمادية)","BRC7EB530 (لوحة قياسية), BRC7F530W (لوحة بيضاء), BRC7F530S (لوحة رمادية)","BRC7EB530 (لوحة قياسية), BRC7F530W (لوحة بيضاء), BRC7F530S (لوحة رمادية)"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standard Accessories","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]