{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":10,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-N9"]
[]
[]
[]
[]
["","","","","FFA25A2VEB9 / RXM25N2V1B9","FFA25A2VEB9 / RXM25N5V1B9","FFA35A2VEB9 / RXM35N2V1B9","FFA35A2VEB9 / RXM35N5V1B9","FFA50A2VEB9 / RXM50N2V1B9","FFA60A2VEB9 / RXM60N2V1B9"]
["Cooling capacity","Nom.","","kW","2.50","2.50"]
["تبريد المساحة","SEER","","","6.17","6.17"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","142","142"]
["","الاستطاعة","Pdesign","kW","2.50","2.50"]
["","فئة فعالية استهلاك الطاقة","","","A++","A++"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","2.31","2.31"]
["","SCOP/A","","","4.24","4.24"]
["","فئة فعالية استهلاك الطاقة","","","A+","A+"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","762","762"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","273","273"]
["","نسبة فعالية استهلاك الطاقة","","","4.57","4.57"]
["","عامل الأداء","","","3.90","3.90"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A"]
["","","تدفئة","","A","A"]
["Heating capacity","Nom.","","kW","3.20","3.20"]
["Notes","","","","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م."]
["","","","","(4) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر.","(4) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["Outdoor unit","","","","","","RXM35N2V1B9","RXM35N5V1B9","","RXM60N2V1B9"]
["Cooling capacity","Nom.","","kW","","","3.40","3.40","5.00","5.70"]
["Heating capacity","Nom.","","kW","","","4.20","4.20","5.80","7.00"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","","","3.81","3.81","3.24","3.05"]
["","عامل الأداء","","","","","3.50","3.50","3.49","3.41"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","","","446","446","772","934"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","","","A","A","A","B"]
["","","تدفئة","","","","B","B","B","B"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","","","A++","A++","A+","A+"]
["","الاستطاعة","Pdesign","kW","","","3.40","3.40","5.00","5.70"]
["","SEER","","","","","6.38","6.38","5.98","5.76"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","186","186","293","347"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","","","A+","A+","A","A+"]
["","الاستطاعة","Pdesign","kW","","","3.10","3.10","3.84","3.96"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","","","4.10","4.10","3.90","4.04"]
["","Pdh استطاعة التدفئة عند -10°","","kW","","","2.04","2.04","3.40","3.66"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","1058","1058","1378","1372"]
["نطاق كفاءة استخدام الطاقة","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]