{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":14,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA60A2VEB9 / FFA60A2VEB9 / RZQG125L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG71L8Y1B"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Cooling capacity","Nom.","","kW","","","","","","","","6.80","6.80","6.80"]
["تبريد المساحة","SEER","","","","","","","","","","5.10","5.10","5.10"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","","","","","","467","467","467"]
["","الاستطاعة","Pdesign","kW","","","","","","","","6.80","6.80","6.80"]
["","فئة فعالية استهلاك الطاقة","","","","","","","","","","A","A","A"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","","","","","","","","6.00","6.00","6.00"]
["","SCOP/A","","","","","","","","","","3.80","3.80","3.80"]
["","فئة فعالية استهلاك الطاقة","","","","","","","","","","A","A","A"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","","","","","","2,211","2,211","2,211"]
["الفعالية الاسمية","نسبة فعالية استهلاك الطاقة","","","","","","","","","","3.38","3.38","3.38"]
["Notes","","","","","","","","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","","","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر.","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","","","","","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","","","","","","","","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]