{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-B9V / RXS-F"]
[]
[]
[]
[]
["","","","","FFQ60B9V1B / RXS60F4V1B","FFQ60B9V1B / RXS60F3V1B"]
["Cooling capacity","Nom.","","كيلوواط","5.80 (3)","5.80 (3)"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","1,035","1,035"]
["","نسبة فعالية استهلاك الطاقة","","","2.80","2.80"]
["","عامل الأداء","","","2.81","2.81"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","D","D"]
["","","تدفئة","","D","D"]
["Heating capacity","Nom.","","كيلوواط","7.00 (4)","7.00 (4)"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)"]
["","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)"]
["","","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","","(5) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]