{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":17,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHA71AVEB / FHA71AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG125L8Y1B","FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA60AVEB / FHA60AVEB / RZQG125L8Y1B","FHA50AVEB / FHA50AVEB / RZQG71L8Y1B","FHA71AVEB / RZQG71L8Y1B","FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA71AVEB / FHA71AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["تبريد المساحة","SEER","","","","","","","","","5.10","6.86","5.10","5.10","5.10","5.10","5.10"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","","","","","","","467","347","467","467","652","652","652"]
["","الاستطاعة","Pdesign","كيلوواط","","","","","","","6.80","6.80","6.80","6.80","9.50","9.50","9.50"]
["","فئة فعالية استهلاك الطاقة","","","","","","","","","A","A++","A","A","A","A","A"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","كيلوواط","","","","","","","6.00","7.60","6.00","6.00","11.30","11.30","11.30"]
["","SCOP/A","","","","","","","","","3.80","4.32","3.80","3.80","3.80","3.80","3.80"]
["","فئة فعالية استهلاك الطاقة","","","","","","","","","A","A+","A","A","A","A","A"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","","","","","","","2,211","2,463","2,211","2,211","4,164","4,164","4,164"]
["Cooling capacity","Nom.","","كيلوواط","","","","","","","","6.80 (1)"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","","","","","","","","890"]
["","نسبة فعالية استهلاك الطاقة","","","","","","","","","","3.82 (3)"]
["","عامل الأداء","","","","","","","","","","4.13 (3)"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","","","","","","","A"]
["","","تدفئة","","","","","","","","","A"]
["Heating capacity","Nom.","","كيلوواط","","","","","","","","7.50 (2)"]
["Notes","","","","","","","","","","","(1) - التبريد: درجة الحرارة الداخلية 27 درجة مئوية للبويصلة الجافة، 19 درجة مئوية للبويصلة الرطبة؛ درجة الحرارة الخارجية 35 درجة مئوية للبويصلة الجافة؛ الطول المكافئ للمواسير: 7.5 متر؛ فرق المستوى: 0 متر","(1) - التبريد: درجة الحرارة الداخلية 27 درجة مئوية للبويصلة الجافة، 19 درجة مئوية للبويصلة الرطبة؛ درجة الحرارة الخارجية 35 درجة مئوية للبويصلة الجافة؛ الطول المكافئ للمواسير: 7.5 متر؛ فرق المستوى: 0 متر"]
["","","","","","","","","","","","(2) - التدفئة: درجة الحرارة الداخلية 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة؛ الطول المكافئ للمواسير: 7.5 متر ؛ فرق المستوى: 0 متر","(2) - التدفئة: درجة الحرارة الداخلية 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة؛ الطول المكافئ للمواسير: 7.5 متر ؛ فرق المستوى: 0 متر"]
["","","","","","","","","","","","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]