{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RXS-F"]
[]
[]
[]
[]
["","","","","FHQ60CAVEB / RXS60F4V1B"]
["Cooling capacity","Nom.","","كيلو واط","5.7"]
["Heating capacity","Nom.","","كيلو واط","7.2"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","3.26"]
["","عامل الأداء","","","3.32"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","875"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","C"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A"]
["","الاستطاعة","Pdesign","كيلو واط","7.20"]
["","SEER","","","5.54"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","360"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A"]
["","الاستطاعة","Pdesign","كيلو واط","5.07"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","3.50"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","2026.36"]