{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":14,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQG-L8/7V1"]
[]
[]
[]
[]
["","","","","FHQ71CAVEB / RZQG71L8V1B","FHQ35CAVEB / FHQ35CAVEB / RZQG71L8V1B","FHQ100CAVEB / RZQG100L8V1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQG100L8V1B","FHQ50CAVEB / FHQ50CAVEB / RZQG100L8V1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQG125L8V1B","FHQ60CAVEB / FHQ60CAVEB / RZQG125L8V1B","FHQ125CAVEB / RZQG125L8V1B","FHQ50CAVEB / FHQ50CAVEB / FHQ50CAVEB / RZQG125L8V1B","FHQ140CAVEB / RZQG140L7V1B"]
["Cooling capacity","Nom.","","كيلوواط","6.8","","9.5","","","","","12.0","","13.4"]
["تبريد المساحة","SEER","","","6.95","5.10","6.11","5.10","5.10","5.10","5.10","6.01","5.10"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","342.446","467","544.19","652","652","824","824","698.835","824"]
["","الاستطاعة","Pdesign","كيلوواط","6.80","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","فئة فعالية استهلاك الطاقة","","","A++","A","A++","A","A","A","A","A+","A"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","كيلوواط","7.60","6.00","11.30","11.30","11.30","12.71","12.71","14.13","12.71"]
["","SCOP/A","","","4.32","3.80","4.61","3.80","3.80","3.80","3.80","4.23","3.80"]
["","فئة فعالية استهلاك الطاقة","","","A+","A","A++","A","A","A","A","A+","A"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","2,462.963","2,211","3,431.67","4,163","4,163","4,683","4,683","4,676.596","4,683"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلوواط ساعي","890","","1,245","","","","","1,790","","2,025"]
["","نسبة فعالية استهلاك الطاقة","","","3.82","","3.81","","","","","3.35","","3.31"]
["","عامل الأداء","","","4.13","","4.15","","","","","3.89","","3.63"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","","A","","","","","A"]
["","","تدفئة","","A","","A","","","","","A"]
["Heating capacity","Nom.","","كيلوواط","7.5","","10.8","","","","","13.5","","15.5"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]