{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Sound pressure level","Heating","","High","dBA","39","40","41","","46"]
["","","","متوسط","dBA","32","33","33","","42"]
["","","","Silent operation","dBA","19","19","19","","24"]
["","","","Low","dBA","25","25","25","","33"]
["","Cooling","","متوسط","dBA","32","33","33","","39"]
["","","","Silent operation","dBA","19","19","19","","24"]
["","","","Low","dBA","25","25","25","","31"]
["","","","High","dBA","39","40","41","","46"]
["Standard Accessories","دليل التركيب","","","","1","1","1","","1"]
["","دليل التشغيل","","","","1","1","1","","1"]
["","مرشح هواء","","","","2","2","2","","2"]
["","جهاز تحكم عن بعد بالأشعة تحت الحمراء","","","","1","1","1","","1"]
["","لوحة تثبيت جهاز التحكم عن بعد","","","","1","1","1","","1"]
["","حقيبة المسامير اللولبية","","","","1","1","1","","1"]
["","غطاء البراغي","","","","1","1","1","","1"]
["","بطاريات جافة قياس AAA","","","","2","2","2","","2"]
["","تدابير السلامة الوقائية العامة","","","","1","1","1","","1"]
["Refrigerant","GWP","","","","675.0","675.0","675.0","","675.0"]
["أنظمة التحكم","Wired remote control","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Piping connections","Liquid","","القطر الخارجي","mm","6.35","6.35","6.35","","6.35"]
["","غاز","","القطر الخارجي","mm","9.50","9.50","9.50","","12.70"]
["","Drain","","","","18","18","18","","18"]
["Power input","Cooling","","Nom.","كيلو واط","0.020","0.022","0.023","","0.030"]
["","Heating","","Nom.","كيلو واط","0.020","0.020","0.022","","0.039"]
["مستوى طاقة الصوت","التبريد","","","dBA","57","57","60","","60"]
["Dimensions","Unit","","العرض","mm","798","798","798","","798"]
["","","","العمق","mm","189","189","189","","189"]
["","","","الارتفاع","mm","295","295","295","","295"]
["الغلاف","اللون","","","","White","White","White","","White"]
["الوزن","الوحدة","","","kg","11.50","11.50","11.50","","11.50"]
["Fan","Air flow rate","التدفئة","High","م³/دقيقة","10.9","11.1","11.5","","15.1"]
["","","","متوسط","م³/دقيقة","8.7","9.0","9.0","","11.1"]
["","","","Low","م³/دقيقة","6.4","6.4","6.4","","8.2"]
["","","","Silent operation","م³/دقيقة","4.5","4.5","4.5","","5.7"]
["","","التبريد","Low","م³/دقيقة","6.1","6.1","6.1","","7.6"]
["","","","متوسط","م³/دقيقة","8.2","8.6","8.6","","10.4"]
["","","","High","م³/دقيقة","11.0","11.5","11.9","","13.5"]
["","","","Silent operation","م³/دقيقة","4.6","4.6","4.6","","5.2"]
["Power supply","الطور","","","","1~","1~","1~","","1~"]
["","الاسم","","","","V1","V1","V1","","V1"]
["","Frequency","","","Hz","50","50","50","","50"]
["","Voltage","","","فولت","220-240","220-240","220-240","","220-240"]
["Power input","Cooling","","Nom.","كيلو واط","","","","0.028"]
["","Heating","","Nom.","كيلو واط","","","","0.036"]
["الغلاف","اللون","","","","","","","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","","","","295"]
["","","","العرض","mm","","","","798"]
["","","","العمق","mm","","","","189"]
["الوزن","الوحدة","","","kg","","","","11.50"]
["Fan","Air flow rate","التبريد","High","م³/دقيقة","","","","13.1"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","م³/دقيقة","","","","9.8"]
["Fan","Air flow rate","التبريد","Low","م³/دقيقة","","","","7.2"]
["","","","Silent operation","م³/دقيقة","","","","4.6"]
["","","التدفئة","High","م³/دقيقة","","","","14.6"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","م³/دقيقة","","","","10.5"]
["Fan","Air flow rate","التدفئة","Low","م³/دقيقة","","","","7.7"]
["","","","Silent operation","م³/دقيقة","","","","5.2"]
["مستوى طاقة الصوت","التبريد","","","dBA","","","","60"]
["Sound pressure level","Cooling","","High","dBA","","","","45"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","","","","37"]
["Sound pressure level","Cooling","","Low","dBA","","","","29"]
["","","","Silent operation","dBA","","","","21"]
["","Heating","","High","dBA","","","","45"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","","","","37"]
["Sound pressure level","Heating","","Low","dBA","","","","29"]
["","","","Silent operation","dBA","","","","21"]
["سائل تبريد","GWP","","","","","","","675.0"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","","","","6.35"]
["","غاز","","القطر الخارجي","mm","","","","12.70"]
["","التصريف","","","","","","","18"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","","","","ARC466A58"]
["","جهاز تحكم عن بُعد سلكي","","","","","","","BRC073"]
["Standard Accessories","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","مرشح هواء","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["وحدة التزويد بالطاقة","الاسم","","","","","","","V1"]
["","الطور","","","","","","","1~"]
["Power supply","Frequency","","","Hz","","","","50"]
["","Voltage","","","فولت","","","","220-240"]