{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":10,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-BS"]
[]
[]
[]
[]
["","","","","","FTXA20B2V1BS","FTXA25B2V1BS","FTXA35B2V1BS","FTXA42B2V1BS","FTXA50B2V1BS"]
["Power input","Cooling","","Nom.","كيلوواط","0.02","0.022","0.023","0.028","0.030"]
["","Heating","","Nom.","كيلوواط","0.02","0.02","0.022","0.036","0.039"]
["الغلاف","اللون","","","","فضة","فضة","فضة","فضة","فضة"]
["الأبعاد","الوحدة","","الارتفاع","مم","295","295","295","295","295"]
["","","","العرض","مم","798","798","798","798","798"]
["","","","العمق","مم","189","189","189","189","189"]
["الوزن","الوحدة","","","kg","11.5","11.5","11.5","11.5","11.5"]
["Fan","Air flow rate","التبريد","High","m³/min","11","11.5","11.9","13.1","13.5"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","8.2","8.6","8.6","9.8","10.4"]
["Fan","Air flow rate","التبريد","Low","m³/min","6.1","6.1","6.1","7.2","7.6"]
["","","","Silent operation","m³/min","4.6","4.6","4.6","4.6","5.2"]
["","","التدفئة","High","m³/min","10.9","11.1","11.5","14.6","15.1"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","8.7","9","9","10.5","11.1"]
["Fan","Air flow rate","التدفئة","Low","m³/min","6.4","6.4","6.4","7.7","8.2"]
["","","","Silent operation","m³/min","4.5","4.5","4.5","5.2","5.7"]
["مستوى طاقة الصوت","التبريد","","","ديسيبل أمبير","57","57","60","60","60"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","39","40","41","45","46"]
["مستوى ضغط الصوت","تبريد","","متوسط","ديسيبل أمبير","32","33","33","37","39"]
["Sound pressure level","Cooling","","Low","ديسيبل أمبير","25","25","25","29","31"]
["","","","Silent operation","ديسيبل أمبير","19","19","19","21","24"]
["","Heating","","High","ديسيبل أمبير","39","40","41","45","46"]
["مستوى ضغط الصوت","تدفئة","","متوسط","ديسيبل أمبير","32","33","33","37","42"]
["Sound pressure level","Heating","","Low","ديسيبل أمبير","25","25","25","29","33"]
["","","","Silent operation","ديسيبل أمبير","19","19","19","21","24"]
["سائل تبريد","GWP","","","","675","675","675","675","675.0"]
["وصلات الأنابيب","سائل","","القطر الخارجي","مم","6.35","6.35","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","مم","9.5","9.5","9.5","12.7","12.70"]
["","التصريف","","","","18","18","18","18","18"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARC466A58","ARC466A58","ARC466A58","ARC466A58","ARC466A58"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC073","BRC073","BRC073","BRC073","BRC073"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","مرشح هواء","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Remote controller mounting plate","","","","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1","V1","V1","V1"]
["","الطور","","","","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240"]