{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CB / RXA-B9"]
[]
[]
[]
[]
["","","","","FTXA42C2V1BB / RXA42B5V1B9"]
["Cooling capacity","Min.","","كيلو واط","1.70"]
["","Nom.","","كيلو واط","4.20"]
["","Max.","","كيلو واط","5.00"]
["Heating capacity","Min.","","كيلو واط","1.70"]
["","Nom.","","كيلو واط","5.40"]
["","Max.","","كيلو واط","6.00"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","3.99"]
["","عامل الأداء","","","4.12"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","526"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A++"]
["","الاستطاعة","Pdesign","كيلو واط","4.20"]
["","SEER","","","7.50"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","196"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A++"]
["","الاستطاعة","Pdesign","كيلو واط","3.80"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","4.60"]
["","Pdh استطاعة التدفئة عند -10°","","كيلو واط","3.04"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","1156"]