{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXLG-M"]
[]
[]
[]
[]
["","","","","FTXG25LV1BW / RXLG25M2V1B","FTXG35LV1BW / RXLG35M2V1B"]
["Cooling capacity","Min.","","كيلوواط","1.3","1.4"]
["","Max.","","كيلوواط","4.0","4.6"]
["","Nom.","","كيلوواط","2.5 (2)","3.5 (2)"]
["Piping connections","Liquid","القطر الخارجي","مم","6.35","6.35"]
["","غاز","القطر الخارجي","مم","9.5","9.5"]
["","Drain","OD","مم","18","18"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","340","490"]
["","نسبة فعالية استهلاك الطاقة","","","3.68 (1)","3.57 (1)"]
["","عامل الأداء","","","4.31 (1)","3.89 (1)"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A"]
["","","تدفئة","","A","A"]
["Heating capacity","Nom.","","كيلوواط","4.4 (2)","5.1 (2)"]
["","Min.","","كيلوواط","1.0 (6)","1.0 (6)"]
["","Max.","","كيلوواط","6.1, 3.6 (7)","6.7, 4.2 (7)"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["","","","","(3) - 220 فولت","(3) - 220 فولت"]
["","","","","(4) - 230 فولت","(4) - 230 فولت"]
["","","","","(5) - 240 فولت","(5) - 240 فولت"]
["","","","","(6) - للحصول على الحد الأدنى المقدّر من استطاعة التدفئة يتم ضبط مروحة الوحدة الداخلية إلى العتبة SL","(6) - للحصول على الحد الأدنى المقدّر من استطاعة التدفئة يتم ضبط مروحة الوحدة الداخلية إلى العتبة SL"]
["","","","","(7) - استطاعة التدفئة الأعظمية عند درجة حرارة خارجية -15° مئوية","(7) - استطاعة التدفئة الأعظمية عند درجة حرارة خارجية -15° مئوية"]