{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 4MXM-A9"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 4MXM80A2V1B9"]
["Cooling capacity","Nom.","","كيلوواط","7.50"]
["Heating capacity","Nom.","","كيلوواط","10.00"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","4.13"]
["","عامل الأداء","","","3.32"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","908"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","C"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A++"]
["","الاستطاعة","Pdesign","كيلوواط","7.50"]
["","SEER","","","6.92"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","380"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A+"]
["","الاستطاعة","Pdesign","كيلوواط","6.46"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","4.02"]
["","Pdh استطاعة التدفئة عند -10°","","كيلوواط","5.28"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","2245"]