{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":14,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / RXJ-M"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / RXJ20M2V1B","FTXJ20MV1BW / RXJ20M5V1B","FTXJ20MV1BW / RXJ20M3V1B","FTXJ25MV1BW / RXJ25M2V1B","FTXJ25MV1BW / RXJ25M3V1B","FTXJ25MV1BW / RXJ25M5V1B","FTXJ35MV1BW / RXJ35M2V1B","FTXJ35MV1BW / RXJ35M5V1B","FTXJ35MV1BW / RXJ35M3V1B","FTXJ50MV1BW / RXJ50MV1B"]
["Cooling capacity","Min.","","كيلوواط","","","1.30","","0.90"]
["","Max.","","كيلوواط","","","2.80","","3.30"]
["","Nom.","","كيلوواط","2.3","2.30","2.30","2.4","2.40","2.40","3.5","3.50","","4.80"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","248","248","248","254","254","254","428","428","","716"]
["","نسبة فعالية استهلاك الطاقة","","","4.64","4.64","4.64","4.73","4.73","4.73","4.09","4.09","","3.35"]
["","عامل الأداء","","","5.00","5.00","5.00","4.57","4.57","4.57","4.04","4.04","","3.65"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A","A","A","A","A","A","","A"]
["","","تدفئة","","A","A","A","A","A","A","A","A","","A"]
["Heating capacity","Nom.","","كيلوواط","2.5","2.5","2.50","3.2","3.20","3.2","4","4.0","","5.80"]
["","Min.","","كيلوواط","","","1.30","","0.90"]
["","Max.","","كيلوواط","","","4.30","","4.70"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["","","","","","(1) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(1) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","(1) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(1) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","(1) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["Cooling capacity","Min.","","كيلوواط","","","","","","","","","0.90"]
["","Nom.","","كيلوواط","","","","","","","","","3.50"]
["","Max.","","كيلوواط","","","","","","","","","4.10"]
["Heating capacity","Min.","","كيلوواط","","","","","","","","","0.90"]
["","Nom.","","كيلوواط","","","","","","","","","4.00"]
["","Max.","","كيلوواط","","","","","","","","","5.10"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","","","","","","","","","4.09"]
["","عامل الأداء","","","","","","","","","","","4.04"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","","","","","","","","","428"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","","","","","","","","","A"]
["","","تدفئة","","","","","","","","","","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","","","","","","","","","A++"]
["","الاستطاعة","Pdesign","كيلوواط","","","","","","","","","3.50"]
["","SEER","","","","","","","","","","","7.19"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","","","","","","","","","170"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","","","","","","","","","A++"]
["","الاستطاعة","Pdesign","كيلوواط","","","","","","","","","3.00"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","","","","","","","","","4.60"]
["","Pdh استطاعة التدفئة عند -10°","","كيلوواط","","","","","","","","","2.61"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","","","","","","","","","913"]