{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / RXJ-N"]
[]
[]
[]
[]
["","","","","FTXJ50MV1BW / RXJ50N2V1B"]
["Cooling capacity","Min.","","كيلوواط","1.40"]
["","Max.","","كيلوواط","5.50"]
["","Nom.","","كيلوواط","4.80"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلوواط ساعي","716"]
["","نسبة فعالية استهلاك الطاقة","","","3.35"]
["","عامل الأداء","","","3.65"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","A"]
["Heating capacity","Nom.","","كيلوواط","5.80"]
["","Min.","","كيلوواط","1.10"]
["","Max.","","كيلوواط","7.00"]
["Notes","","","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0"]
["","","","","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]