{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":14,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M / 4MXM-N"]
[]
[]
[]
[]
["","","","","FTXM20M2V1B / FTXM20M2V1B / FTXM25M2V1B / 4MXM68N2V1B","FTXM25M2V1B / FTXM42M2V1B / 4MXM68N2V1B","FTXM20M2V1B / FTXM25M2V1B / FTXM25M2V1B / 4MXM68N2V1B","FTXM20M2V1B / FTXM50M2V1B / 4MXM68N2V1B","FTXM35M2V1B / FTXM35M2V1B / 4MXM68N2V1B","FTXM20M2V1B / FTXM20M2V1B / FTXM20M2V1B / FTXM20M2V1B / 4MXM80N2V1B","FTXM20M2V1B / FTXM60M2V1B / 4MXM80N2V1B","FTXM35M2V1B / FTXM42M2V1B / 4MXM80N2V1B","FTXM20M2V1B / FTXM20M2V1B / FTXM42M2V1B / 4MXM80N2V1B","FTXM20M2V1B / FTXM25M2V1B / FTXM35M2V1B / 4MXM80N2V1B"]
["Cooling capacity","Nom.","","كيلوواط","6.5","6.7","6.8","6.8","6.8","7.40","7.40","7.70","8.00","7.40"]
["تبريد المساحة","SEER","","","7.76","7.99","7.71","7.78","8.02","8.32","7.38","7.40","8.07","8.19"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","294","294","309","306","297","311","351","365","356","317"]
["","الاستطاعة","Pdesign","كيلوواط","6.50","6.70","6.80","6.80","6.80","7.40","7.40","7.70","8.20","7.40"]
["","فئة فعالية استهلاك الطاقة","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","كيلوواط","5.30","4.30","5.30","4.50","4.80","6.23","4.27","4.27","5.37","5.37"]
["","SCOP/A","","","4.09","3.86","4.10","3.90","4.00","4.55","4.05","4.05","3.93","3.95"]
["","فئة فعالية استهلاك الطاقة","","","A+","A","A+","A","A+","A+","A+","A+","A","A"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","1,814","1,559","1,807","1,612","1,680","1,915","1,474","1,475","1,913","1,902"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","810","751","883","794","723","810","803","841","874","749"]
["","نسبة فعالية استهلاك الطاقة","","","4.01","4.46","3.85","4.28","4.70","4.57","4.61","4.58","4.58","4.94"]
["","عامل الأداء","","","4.49","3.95","4.38","3.82","3.81","4.97","3.85","3.35","3.91","3.90"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A","A","A","A","A","A","A","A"]
["","","تدفئة","","A","A","A","A","A","A","A","C","A","A"]
["Heating capacity","Nom.","","كيلوواط","8.20","8.30","8.60","8.60","8.60","9.60","9.30","9.00","9.40","9.30"]
["Notes","","","","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]