{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":11,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / 3MXM-A9"]
[]
[]
[]
[]
["","","","","FTXM20N2V1B / FTXM20N2V1B / 3MXM40A2V1B9","FTXM25N2V1B / FTXM25N2V1B / 3MXM52A2V1B9","FTXM25N2V1B / FTXM42N2V1B / 3MXM68A2V1B9","FTXM35N2V1B / FTXM35N2V1B / 3MXM68A2V1B9","FTXM20N2V1B / FTXM50N2V1B / 3MXM68A2V1B9","FTXM20N2V1B / FTXM25N2V1B / FTXM25N2V1B / 3MXM68A2V1B9","FTXM20N2V1B / FTXM20N2V1B / FTXM25N2V1B / 3MXM68A2V1B9"]
["Cooling capacity","Nom.","","kW","4.00","5.00","6.70","6.80","6.80","6.80","6.50"]
["Heating capacity","Nom.","","kW","4.60","6.80","8.30","8.60","8.60","8.60","8.20"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","4.76","4.85","3.74","3.94","3.59","3.85","4.01"]
["","عامل الأداء","","","4.73","4.45","3.95","3.81","3.82","4.38","4.49"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي","420","515","896","863","947","883","810"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A","A","A","A","A"]
["","","تدفئة","","A","A","A","A","A","A","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A+++","A+++","A++","A++","A++","A++","A++"]
["","الاستطاعة","Pdesign","kW","4.00","5.00","6.70","6.80","6.80","6.80","6.50"]
["","SEER","","","8.53","8.59","6.94","6.97","6.75","7.71","7.76"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","165","204","338","342","352","309","294"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A+","A+","A","A+","A","A+","A+"]
["","الاستطاعة","Pdesign","kW","4.80","4.80","4.30","4.80","4.50","5.30","5.30"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","4.24","4.38","3.86","4.00","3.90","4.10","4.09"]
["","Pdh استطاعة التدفئة عند -10°","","kW","3.60","3.90","3.41","3.73","3.55","4.22","4.21"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","1582","1533","1559","1680","1612","1807","1814"]