{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RXS-F"]
[]
[]
[]
[]
["","","","","FTXS60GV1B / RXS60F4V1B","FTXS60GV1B / RXS60F3V1B","FTXS71GV1B / RXS71FAV1B","FTXS71GV1B / RXS71FAV1B9"]
["Cooling capacity","Min.","","كيلوواط","1.7","1.7","2.3","2.3"]
["","Max.","","كيلوواط","6.7","6.7","8.5","8.5"]
["","Nom.","","كيلوواط","6.0 (2)","6.0 (3)","7.1 (3)","7.1 (2)"]
["Piping connections","Liquid","القطر الخارجي","مم","6.35","6.35","6.35","6.35"]
["","غاز","القطر الخارجي","مم","12.7","12.7","15.9","15.9"]
["","Drain","OD","مم","18.0","18.0","18.0","18.0"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","995","995","1,175","1,175"]
["","نسبة فعالية استهلاك الطاقة","","","3.02","3.02","3.02","3.02"]
["","عامل الأداء","","","3.43","3.43","3.22","3.22"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","B","B","B","B"]
["","","تدفئة","","B","B","C","C"]
["Heating capacity","Nom.","","كيلوواط","7.0 (3)","7.0 (4)","8.2 (4)","8.2 (3)"]
["","Min.","","كيلوواط","1.7","1.7","2.3","2.3"]
["","Max.","","كيلوواط","8.0","8.0","10.2","10.2"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(4) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["","","","","","(5) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(5) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]