{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RXS-L"]
[]
[]
[]
[]
["","","","","FTXS60GV1B / RXS60L2V1B"]
["Cooling capacity","Min.","","kW","1.7"]
["","Nom.","","kW","6.0"]
["","Max.","","kW","6.7"]
["Heating capacity","Min.","","kW","1.7"]
["","Nom.","","kW","7.0"]
["","Max.","","kW","8.0"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","3.02"]
["","عامل الأداء","","","3.43"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي","995"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","B"]
["","","تدفئة","","B"]
["Piping connections","Drain","OD","mm","18"]
["وصلات الأنابيب","غاز","القطر الخارجي","mm","12.7"]
["","سائل","القطر الخارجي","mm","6.35"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A"]
["","الاستطاعة","Pdesign","kW","6.00"]
["","SEER","","","5.58"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","376"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A"]
["","الاستطاعة","Pdesign","kW","4.80"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","3.89"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","1728"]
["Notes","","","","(1) - 220 فولت"]
["","","","","(2) - 230 فولت"]
["","","","","(3) - 240 فولت"]