{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Sound pressure level","Heating","","High","ديسيبل أمبير","38","39","42","42","44","","46"]
["","","","Silent operation","ديسيبل أمبير","25","25","26","30","31","","34"]
["","","","Low","ديسيبل أمبير","28","28","29","33","34","","37"]
["","Cooling","","Silent operation","ديسيبل أمبير","22","22","23","30","31","","34"]
["","","","Low","ديسيبل أمبير","25","25","26","33","34","","37"]
["","","","High","ديسيبل أمبير","38","38","42","42","43","","46"]
["","","","Nom.","ديسيبل أمبير","33","34","36","38","39","","42"]
["","Cooling","","Nom.","ديسيبل أمبير","32","32","34","38","39","","42"]
["Standard Accessories","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم","","","","2","2","2","2","2"]
["","دليل التشغيل","","","","1","1","1","1","1","","1"]
["","دليل التركيب","","","","1","1","1","1","1","","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","1","1","1","1","1","","1"]
["","البطاريات","","","","2","2","2","2","2","","2"]
["","حامل جهاز التحكم عن بعد","","","","1","1","1","1","1","","1"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2","2","2","2","2","","2"]
["","لوح التثبيت","","","","1","1","1","1","1","","1"]
["أنظمة التحكم","Infrared remote control","","","","","","","","","","ARC452A3"]
["Piping connections","Liquid","","القطر الخارجي","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","غاز","","القطر الخارجي","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Drain","","","","18","18","18","18","18","","18"]
["Power input","Cooling","","Nom.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Heating","","Nom.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Sound power level","التبريد","","","ديسيبل أمبير","54","54","58","58","59","","63"]
["","التدفئة","","","ديسيبل أمبير","54","55","58","58","60","","62"]
["Dimensions","Unit","","العرض","mm","800","800","800","800","800","","1,050"]
["","","","العمق","mm","215","215","215","215","215","","250"]
["","","","الارتفاع","mm","295","295","295","295","295","","290"]
["تغليف","Colour","","","","White","White","White","White","White","","White"]
["الوزن","الوحدة","","","kg","9","9","10","10","10","","12"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","","1~"]
["","Frequency","","","Hz","50","50","50","50","50","","50"]
["","الاسم","","","","V1","V1","V1","V1","V1","","V1"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء"]
["","","","","","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت","(2) - 220 فولت"]
["","","","","","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت","(3) - 230 فولت"]
["Fan","Air flow rate","التبريد","Nom.","m³/min","","","","","","16.0"]
["Sound pressure level","Cooling","","Nom.","ديسيبل أمبير","","","","","","41"]
["Fan","Air flow rate","التدفئة","Nom.","m³/min","","","","","","14.9"]
["Sound pressure level","Heating","","Nom.","ديسيبل أمبير","","","","","","40"]
["Power input","Cooling","","Nom.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Heating","","Nom.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["الغلاف","اللون","","","","","","","","","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","","","","","","290"]
["","","","العرض","mm","","","","","","1050"]
["","","","العمق","mm","","","","","","250"]
["الوزن","الوحدة","","","kg","","","","","","12"]
["Fan","Air flow rate","التبريد","High","m³/min","","","","","","16.0"]
["","","","Low","m³/min","","","","","","11.3"]
["","","","Silent operation","m³/min","","","","","","10.1"]
["","","التدفئة","High","m³/min","","","","","","17.2"]
["","","","Low","m³/min","","","","","","12.6"]
["","","","Silent operation","m³/min","","","","","","11.3"]
["مستوى طاقة الصوت","التبريد","","","ديسيبل أمبير","","","","","","60"]
["","التدفئة","","","ديسيبل أمبير","","","","","","59"]
["Sound pressure level","Cooling","","High","ديسيبل أمبير","","","","","","45"]
["","","","Low","ديسيبل أمبير","","","","","","36"]
["","","","Silent operation","ديسيبل أمبير","","","","","","33"]
["","Heating","","High","ديسيبل أمبير","","","","","","44"]
["","","","Low","ديسيبل أمبير","","","","","","35"]
["","","","Silent operation","ديسيبل أمبير","","","","","","32"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","","","","","","6.35"]
["","غاز","","القطر الخارجي","mm","","","","","","12.7"]
["","التصريف","","","","","","","","","18"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","","","","","","ARC452A3"]
["Standard Accessories","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["وحدة التزويد بالطاقة","الاسم","","","","","","","","","V1"]
["","الطور","","","","","","","","","1~"]
["Power supply","Frequency","","","Hz","","","","","","50"]
["","Voltage","","","V","","","","","","220-240"]
["Standard Accessories","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم بدون إطار","","","","","","","","","","2"]
["Notes","","","","","","","","","","","(4) - 240 فولت"]