{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Sound pressure level","Heating","","High","ديسيبل أمبير","39","42","44"]
["","","","Silent operation","ديسيبل أمبير","19","19","24"]
["","","","Low","ديسيبل أمبير","28","29","31"]
["","Cooling","","Silent operation","ديسيبل أمبير","19","19","23"]
["","","","Low","ديسيبل أمبير","26","27","30"]
["","","","High","ديسيبل أمبير","38","42","47"]
["","","","Nom.","ديسيبل أمبير","35","36","38"]
["","Cooling","","Nom.","ديسيبل أمبير","33","35","38"]
["Standard Accessories","مرشح تنقية الهواء وإزالة الروائح بالتحفيز الضوئي","","","","1","1","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","1","1","1"]
["","بطاريات جافة","","","","2","2","2"]
["","حامل جهاز التحكم عن بعد","","","","1","1","1"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","3","3","3"]
["","لوح التثبيت","","","","1","1","1"]
["أنظمة التحكم","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Piping connections","Liquid","","القطر الخارجي","mm","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.5","9.5","9.5"]
["Power input","Cooling","","Nom.","كيلوواط","0.030","0.030","0.030"]
["","Heating","","Nom.","كيلوواط","0.030","0.030","0.030"]
["Sound power level","التبريد","","","ديسيبل أمبير","54","57","60"]
["","التدفئة","","","ديسيبل أمبير","56","57","59"]
["Dimensions","Unit","","العرض","mm","798","798","798"]
["","","","العمق","mm","372","372","372"]
["","","","الارتفاع","mm","295","295","295"]
["الغلاف","اللون","","","","White","White","White"]
["الوزن","الوحدة","","","kg","15","15","15"]
["Fan","Air flow rate","Heating","High","m³/min","11.7","13.3","14.4"]
["","","","Low","m³/min","6.7","6.9","7.7"]
["","","","Silent operation","m³/min","4.8","4.8","5.9"]
["","","Cooling","Low","m³/min","5.3","5.6","6.6"]
["","","","High","m³/min","10.7","12.1","15.0"]
["","","","Silent operation","m³/min","4.0","4.0","4.6"]
["","","","Nom.","m³/min","8.6","9.2","10.7"]
["","","Cooling","Nom.","m³/min","7.5","8.4","9.2"]
["Power supply","الطور","","","","1~","1~","1~"]
["","الاسم","","","","V1","V1","V1"]
["","Frequency","","","هرتز","50","50","50"]
["","Voltage","","","فولت","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - 220 فولت","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت","(2) - 230 فولت","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت","(3) - 240 فولت","(3) - 240 فولت"]
["","","","","","(4) - الجهة الأمامية للمبادل الحراري","(4) - الجهة الأمامية للمبادل الحراري","(4) - الجهة الأمامية للمبادل الحراري"]
["","","","","","(5) - الجهة الخلفية للمبادل الحراري","(5) - الجهة الخلفية للمبادل الحراري","(5) - الجهة الخلفية للمبادل الحراري"]