{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":16,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUA100AVEB / RZQG100L8Y1B","FUA125AVEB / RZQG125L8Y1B","FUA71AVEB / FUA71AVEB / RZQG100L8Y1B","FUA71AVEB / FUA71AVEB / RZQG125L8Y1B","FUA100AVEB9 / RZQG100L8Y1B","FUA125AVEB9 / RZQG125L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG100L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG125L8Y1B","FUA71AVEB / RZQG71L8Y1B","FUA100AVEB / RZQG71L8Y1B","FUA71AVEB9 / RZQG71L8Y1B","FUA100AVEB9 / RZQG71L8Y1B"]
["Cooling capacity","Nom.","","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["تبريد المساحة","SEER","","","","","","","","","","","6.42","6.42","6.42","6.42"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","","","","","","","","","371","371","371","371"]
["","الاستطاعة","Pdesign","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["","فئة فعالية استهلاك الطاقة","","","","","","","","","","","A++","A++","A++","A++"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","","","","","","","","","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","","","","","","","","","4.20","4.20","4.20","4.20"]
["","فئة فعالية استهلاك الطاقة","","","","","","","","","","","A+","A+","A+","A+"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","","","","","","","","","2,534","2,534","2,534","2,534"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","كيلو واط ساعي","","","","","","","","","835","","835"]
["","نسبة فعالية استهلاك الطاقة","","","","","","","","","","","4.07","4.07","4.07","4.07"]
["","عامل الأداء","","","","","","","","","","","4.08","","4.08"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","","","","","","","","A","","A"]
["","","تدفئة","","","","","","","","","","A","","A"]
["Heating capacity","Nom.","","kW","","","","","","","","","7.50","","7.50"]
["Notes","","","","","","","","","","","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","","","","","","","","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر.","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(2) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر.","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","","","","","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل","","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","","","","","","","","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","","(4) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]