{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Sound pressure level","Heating","","High","dBA","","","","41","46","47"]
["","","","متوسط","dBA","","","","38","42","43"]
["","","","Low","dBA","","","","35","39","40"]
["","Cooling","","متوسط","dBA","","","","38","42","43"]
["","","","Low","dBA","","","","35","39","40"]
["","","","High","dBA","","","","41","46","47"]
["Standard Accessories","دليل التشغيل","","","","","","","1","1","1"]
["","دليل التركيب","","","","","","","1","1","1"]
["","خرطوم الصرف","","","","","","","1","1","1"]
["","أنبوب العزل الحراري","","","","","","","3","3","3"]
["","أغلفة برباط","","","","","","","10","10","10"]
["","حلقة تثبيت الخرطوم","","","","","","","1","1","1"]
["","مواد مانعة للتسريب","","","","","","","4","4","4"]
["","حلقة للوحة التثبيت","","","","","","","1","1","1"]
["","وصلة تصريف","","","","","","","1","1","1"]
["","قماش غير منسوج","","","","","","","1","1","1"]
["","حلقة إحكام الربط","","","","","","","8","8","8"]
["","مسمار تثبيت لولبي لخرطوم الصرف","","","","","","","5","5","5"]
["أنظمة التحكم","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Cooling capacity","Total capacity","","Nom.","kW","","","","","","12.1"]
["Piping connections","Liquid","","القطر الخارجي","mm","","","","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","","","","15.9","15.9","15.9"]
["","Drain","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","التبريد","","","dBA","","","","59","64","65"]
["","التدفئة","","","dBA","","","","59","64"]
["Dimensions","Unit","","العرض","mm","","","","950","950","950"]
["","","","العمق","mm","","","","950","950","950"]
["","","","الارتفاع","mm","","","","198","198","198"]
["الغلاف","المادة","","","","","","","Resin","Resin","Resin"]
["","اللون","","","","","","","أبيض صاف","أبيض صاف","أبيض صاف"]
["الوزن","الوحدة","","","kg","","","","25.0","26.0","26"]
["Fan","Air flow rate","Heating","High","m³/min","","","","23.0","31.0","32.5"]
["","","","متوسط","m³/min","","","","19.5","25.5","26.5"]
["","","","Low","m³/min","","","","16.0","20.0","20.5"]
["","","Cooling","Low","m³/min","","","","16.0","20.0","20.5"]
["","","","متوسط","m³/min","","","","19.5","25.5","26.5"]
["","","","High","m³/min","","","","23.0","31.0","32.5"]
["ارتفاع الصرف","mm","","","","","","","600","600","600"]
["Heating capacity","الاستطاعة الإجمالية","","الإسمي","kW","","","","","","13.5"]
["الغلاف","اللون","","","","أبيض صاف","أبيض صاف","أبيض صاف"]
["","المادة","","","","Resin","Resin","Resin"]
["الأبعاد","الوحدة","","الارتفاع","mm","198","198","198"]
["","","","العرض","mm","950","950","950"]
["","","","العمق","mm","950","950","950"]
["الوزن","الوحدة","","","kg","25.0","26.0","26.0"]
["Fan","Air flow rate","Cooling","High","m³/min","23.0","31.0","32.5"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","19.5","25.5","26.5"]
["Fan","Air flow rate","Cooling","Low","m³/min","16.0","20.0","20.5"]
["","","Heating","High","m³/min","23.0","31.0","32.5"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","19.5","25.5","26.5"]
["Fan","Air flow rate","Heating","Low","m³/min","16.0","20.0","20.5"]
["مستوى طاقة الصوت","التبريد","","","dBA","59","64","65"]
["Sound pressure level","Cooling","","High","dBA","41","46","47"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","38","42","43"]
["Sound pressure level","Cooling","","Low","dBA","35","39","40"]
["","Heating","","High","dBA","41","46","47"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","38","42","43"]
["Sound pressure level","Heating","","Low","dBA","35","39","40"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.9","15.9","15.9"]
["","التصريف","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["ارتفاع الصرف","mm","","","","600","600","600"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Cooling capacity","Total capacity","","Nom.","kW","","","12.10"]
["استطاعة التدفئة","الاستطاعة الإجمالية","","الإسمي","kW","","","13.5"]