{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C"]
[]
[]
[]
[]
["","","","","FUQ71CVEB","FUQ100CVEB","FUQ125CVEB"]
["Sound pressure level","Heating","High","ديسيبل أمبير","41","46","47"]
["","","Nom.","ديسيبل أمبير","38","42","43"]
["","","Low","ديسيبل أمبير","35","39","40"]
["","Cooling","Low","ديسيبل أمبير","35","39","40"]
["","","High","ديسيبل أمبير","41","46","47"]
["","","Nom.","ديسيبل أمبير","38","42","43"]
["Standard Accessories","Installation manual","","","Installation manual","Installation manual","Installation manual"]
["","Operation manual","","","Operation manual","Operation manual","Operation manual"]
["","إعلان التوافق","","","إعلان التوافق","إعلان التوافق","إعلان التوافق"]
["","خرطوم الصرف","","","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف"]
["","مشبك معدني","","","مشبك معدني","مشبك معدني","مشبك معدني"]
["","حلقة للدعامة الحاملة","","","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة"]
["","مشابك","","","مشابك","مشابك","مشابك"]
["","حلقة إحكام الربط","","","حلقة إحكام الربط","حلقة إحكام الربط","حلقة إحكام الربط"]
["","مادة عازلة ومانعة تسريب للوصلات","","","مادة عازلة ومانعة تسريب للوصلات","مادة عازلة ومانعة تسريب للوصلات","مادة عازلة ومانعة تسريب للوصلات"]
["","كوع","","","كوع","كوع","كوع"]
["","نموذج التركيب","","","نموذج التركيب","نموذج التركيب","نموذج التركيب"]
["","مادة مانعة","","","مادة مانعة","مادة مانعة","مادة مانعة"]
["","أنبوب منحني بشكل L","","","أنبوب منحني بشكل L","أنبوب منحني بشكل L","أنبوب منحني بشكل L"]
["","مسامير لولبية","","","مسامير لولبية","مسامير لولبية","مسامير لولبية"]
["","قماش غير منسوج","","","قماش غير منسوج","قماش غير منسوج","قماش غير منسوج"]
["أنظمة التحكم","جهاز تحكم عن بُعد سلكي","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7C58","BRC7C58","BRC7C58"]
["Piping connections","Liquid","القطر الخارجي","mm","9.52","9.52","9.52"]
["","غاز","القطر الخارجي","mm","15.9","15.9","15.9"]
["","Drain","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","التبريد","","ديسيبل أمبير","59","64","65"]
["","التدفئة","","ديسيبل أمبير","59","64","65"]
["Dimensions","Unit","العرض","mm","950","950","950"]
["","","العمق","mm","950","950","950"]
["","","الارتفاع","mm","198","198","198"]
["الغلاف","المادة","","","Resin","Resin","Resin"]
["","Colour","","","أبيض صاف","أبيض صاف","أبيض صاف"]
["الوزن","الوحدة","","كغ","25","26","26"]
["ارتفاع الصرف","mm","","","600","600","600"]
["Power supply","Phase","","","1~","1~","1~"]
["","Frequency","","هرتز","50/60","50/60","50/60"]
["","الاسم","","","VE","VE","VE"]
["","Voltage","","V","220-240/220","220-240/220","220-240/220"]