{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A / RZAG-MV1"]
[]
[]
[]
[]
["","","","","FVA100AMVEB / RZAG71M7V1B","FVA71AMVEB / RZAG71M7V1B","FVA140AMVEB / RZAG100M7V1B","FVA100AMVEB / RZAG100M7V1B","FVA125AMVEB / RZAG125M7V1B","FVA140AMVEB / RZAG140M7V1B"]
["Cooling capacity","Nom.","","kW","","6.80 (1)","9.50 (1)","9.50 (1)","12.1 (1)","13.4 (1)"]
["تبريد المساحة","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","","374","517","554","1,133","1,314"]
["","الاستطاعة","Pdesign","kW","","6.80","9.50","9.50","12.1","13.4"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","","4.70","7.80","7.80","9.52","9.52"]
["","استهلاك الطاقة السنوي","","كيلوواط ساعي/سنة","","1,625","2,697","2,600","3,209","3,383"]
["Heating capacity","Nom.","","kW","","7.50 (2)","10.8 (2)","10.8 (2)","13.5 (2)","15.5 (2)"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D"]
["تبريد المساحة","SEER","","","","6.37","6.43","6.00","6.41","6.12"]
["","فئة فعالية استهلاك الطاقة","","","","A++","A++","A+"]
["تدفئة المساحة (مناخ معتدل)","SCOP/A","","","","4.05","4.05","4.20","4.15","3.94"]
["","فئة فعالية استهلاك الطاقة","","","","A+","A+","A+"]
["Notes","","","","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - التبريد: T2: درجة الحرارة الداخلية 26,6‏° مئوية CDB، و19,4‏° مئوية CWB، درجة الحرارة الخارجية 48°CDB [وحدة حرارية/ساعة/واط]","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م."]
["","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(3) - انظر الرسم المنفصل لنطاق التشغيل","","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل","(3) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(4) - See separate drawing for electrical data","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]